>> MIB - Management Information Base
>> Table: voipSipDialTable - (.1.3.6.1.4.1.272.4.33.6.18.1)
Description: Contains the elements of a (backup) dial entry.
voipSipDialTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Rule | DisplayString | RW
.4 | Account | INTEGER | RW
.5 | Next | INTEGER | RW
Index
Unique index of entry.
AdminStatus
Administrative status for dial/backup entry: 'enable' -> the entry is active; 'disable' -> the entry will be ignored. Deafult value is enable. Enumerations: enable (1) disable (2) new (3) delete (8)
Rule
Manipulation rule for dialed number. The string format of a manipulation rule is '<x:y>' (lenghts of strings x and y can vary). A rule entry can contain multiple manipulation rules separated by ';'. The best matching manipulation rule of a rule entry gets used. Length: 0 to 100
Account
Table index number of an interface/account/line used for dialing. That can be either a caller's ISDN or analog interface (on this gateway), a voipSipLineTable entry or a SIP provider account. For table index number range see 'SrcIf' of voipSipRouteTable.
Next
Next dial entry in the priority list. If the connection failed with a provider error, the entry refrenced by this index is used for next dial attempt. So unlimited routes can be created and sorted to user defined fallback solutions.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH