>> MIB - Management Information Base
>> Table: atmOamStatTable - (.1.3.6.1.4.1.272.4.16.14.1)
Description: This tables displays all used VCs.
atmOamStatTable
OID | Name | Type | Access
.1 | AtmIfIndex | INTEGER | R
.2 | Vpi | INTEGER | R
.3 | Vci | INTEGER | R
.4 | FlowType | ENUM | R
.6 | LoopbackTxCells | Counter | R
.7 | LoopbackRxCells | Counter | R
.8 | LoopbackPending | Counter | R
.9 | LoopbackCorr | INTEGER | R
.10 | AisState | ENUM | R
.11 | AisTxCells | Counter | R
.12 | AisRxCells | Counter | R
.13 | TotalAisTxCells | Counter | R
.14 | TotalAisRxCells | Counter | R
.15 | RdiState | ENUM | R
.16 | RdiTxCells | Counter | R
.17 | RdiRxCells | Counter | R
.18 | TotalRdiTxCells | INTEGER | R
.19 | TotalRdiRxCells | Counter | R
.20 | CCActivatorState | ENUM | R
.21 | CCActivatorDirection | ENUM | R
.22 | CCActivatorCorr | INTEGER | R
.23 | CCResponderState | ENUM | R
.24 | CCResponderDirection | ENUM | R
.25 | CCResponderCorr | INTEGER | R
.26 | CCTxCells | Counter | R
.27 | CCRxCells | Counter | R
AtmIfIndex
The interface index of the associated ATM hardware.
Vpi
The VPI value of this Virtual Path Connection. Range: 0 to 255
Vci
The VCI value of this Virtual Channel Connection. Range: 0 to 65535
FlowType
The OAM hierarchical flow levels: see ITU I.610 Enumerations: f5-segment (1) f5-end2end (2) f4-segment (3) f4-end2end (4)
LoopbackTxCells
The number of OAM loopback cells that have been sent to the target in this sequence.
LoopbackRxCells
The number of OAM loopback cells that have been received from the target in this sequence.
LoopbackPending
The number of currently outstanding OAM loopback responses.
LoopbackCorr
The correlation of the last sent loopback message.
AisState
The AIS state is set to on(2) after receiving an AIS cell or detection of LOC (Loss of Continuity). The Ais state is set to off(1) either when receiving user cells (same VCC context) or via timeout. Enumerations: off (1) on (2)
AisTxCells
The number of OAM alarm indication signal (AIS) cells that have been transmitted since last change of AisState.
AisRxCells
The number of OAM alarm indication signal (AIS) cells that have been received since last change of AisState.
TotalAisTxCells
The total number of OAM alarm indication signal (AIS) cells that have been transmitted.
TotalAisRxCells
The total number of OAM alarm indication signal (AIS) cells that have been received.
RdiState
The RDI state is set to on(2) after receiving a RDI cell. The RDI state is to off(1) via timeout. Enumerations: off (1) on (2)
RdiTxCells
The number of OAM remote defect indication (RDI) cells that have been transmitted since last change of RdiState.
RdiRxCells
The number of OAM remote defect indication (RDI) cells that have been received since last change of RdiState.
TotalRdiTxCells
The totoal number of OAM remote defect indication (RDI) cells that have been transmitted.
TotalRdiRxCells
The total number of OAM remote defect indication (RDI) cells that have been received.
CCActivatorState
The status of the initiated CC negotiation, inactive(1) is the initial status, wait-act-con(2) is set after sending an CC activation request, active(3) is reached after receiving the CC activation confirmation whereas wait-deact-con(4) is used to indicate awaiting the CC deactivation confirmation. Enumerations: inactive (1) wait-act-con (2) active (3) wait-deact-con (4)
CCActivatorDirection
The direction of action indicated by a received CC activation confirmation, source(1) correlates with 'A-B', sink(2) with 'B-A' and both(3) with 'A-B' and 'B-A'. Enumerations: sink (1) source (2) both (3) not-applicable (4)
CCActivatorCorr
The correlation of the last CC activation message sent to the responder.
CCResponderState
The status of the passive CC negotiation, inactive(1) is the initial status, active(3) is reached after receiving an CC activation request whereas wait-deact-con(4) is used to indicate awaiting the CC deactivation confirmation. Enumerations: inactive (1) active (3) wait-deact-con (4)
CCResponderDirection
The direction of action indicated by a received CC activation request, source(1) correlates with 'B-A', sink(2) with 'A-B' and both(3) with 'A-B' and 'B-A'. Enumerations: source (1) sink (2) both (3) not-applicable (4)
CCResponderCorr
The correlation of the received CC activation message.
CCTxCells
The number of OAM continuity check cells that have been sent to the target in this sequence.
CCRxCells
The number of OAM continuity check cells that have been received from the target in this sequence.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH