>> MIB - Management Information Base
>> Table: httpAdmin - (.1.3.6.1.4.1.272.4.22.5.1)
httpAdmin
OID | Name | Type | Access
.2 | SPort | INTEGER | RW
.3 | Timeout | INTEGER | RW
.4 | KeepAlive | ENUM | RW
.5 | KeepAliveTimeout | INTEGER | RW
.6 | MaxKeepAliveRequests | INTEGER | RW
.7 | SessionTimeout | INTEGER | RW
.8 | LoginMaxFailed | INTEGER | RW
.9 | LoginFailedDelay | INTEGER | RW
.10 | MaxSessions | INTEGER | RW
.11 | CertIndex | INTEGER | RW
.12 | OspPort | INTEGER | RW
SPort
HTTPS server port. Range: 0 to 65535
Timeout
HTTP server timeout in seconds. Range: 30 to 3600
KeepAlive
Allow persistent connections (more than one request per connection) true : allowed false: not allowed Enumerations: true (1) false (2)
KeepAliveTimeout
Number of seconds to wait for the next request from the same client on the same connection. Range: 5 to 60
MaxKeepAliveRequests
The maximum number of requests to allow during a persistent connection. Set to 0 to allow an unlimited amount. We recommend you leave this number high, for maximum performance. Range: 0 to 10000
SessionTimeout
The number of seconds until a session is timed out on inactivity. Range: 300 to 86400
LoginMaxFailed
The number of failed HTTP session (wrong authentication), that causes the next session with delayed acceptance. Range: 0 to 255
LoginFailedDelay
The number of seconds a new session is delayed (not accepted) if httpAdminLoginMaxFailed was reached. Range: 3 to 255
MaxSessions
The maximum number of HTTP(S)-sessions allowed in parallel. Range: 1 to 1000
CertIndex
The index of the certificate to use (from the certTable) for HTTPS sessions. If 0, predefined certificate is used.
OspPort
HTTPS OpenStage server port. Range: 0 to 65535

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH