>> MIB - Management Information Base
>> Table: capiInfoTable - (.1.3.6.1.4.1.272.4.7.5.1)
Description: The capiInfoTable contains the last 10 CAPI info codes and their message identifiers for where the error occured. The most recent message is at inx 09 with older messages rolling off the top of the table, i.e. inx 00. Creating entries: Entries are created automatically by the system once a CAPI info code is received by a registered application. Deleting entries: Entries are removed automatically by the system.
capiInfoTable
OID | Name | Type | Access
.1 | Application | INTEGER | R
.2 | Plci | HexValue | R
.3 | Ncci | HexValue | R
.4 | C1Command | ENUM | R
.5 | C2Command | ENUM | R
.6 | SubCommand | ENUM | R
.7 | Number | HexValue | R
Application
The application number (capiApplNumber).
Plci
The CAPI PLCI number (capiPlciNumber). Range: 0 to -1
Ncci
The NCCI number (capiNcciNumber). Range: 0 to -1
C1Command
The CAPI 1.1 command where the info occurred. Enumerations: resetb3 (1) connect (2) conact (3) disc (4) listen (5) param (6) info (7) data (8) conninfo (9) dtmf (10) selb2 (64) selb3 (128) listenb3 (129) conb3 (130) conb3act (131) discb3 (132) b3param (133) datab3 (134) handset (135)
C2Command
The CAPI 2.0 command where the info occurred. Enumerations: alert (1) connect (2) conact (3) disc (4) listen (5) info (8) selectb (65) facility (128) conb3 (130) conb3act (131) discb3 (132) datab3 (134) resetb3 (135) conb3t90 (136) manufact (255)
SubCommand
The CAPI 1.1/2.0 subcommand. Enumerations: req (1) conf (2) ind (3) resp (4)
Number
The info value as specified in the CAPI 1.1/2.0 specification. See the Software Reference Manual for a listing of CAPI 1.1 and CAPI 2.0 info values. Range: 0 to -1

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH