>> MIB - Management Information Base
>> Table: wlanWDSStatsTable - (.1.3.6.1.4.1.272.4.46.24.1)
Description: WDS Link Statistics
wlanWDSStatsTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | MSDUTx | Counter32 | R
.3 | MSDURx | Counter32 | R
.4 | BytesTx | Counter32 | R
.5 | BytesRx | Counter32 | R
.6 | CurrentRate | WlanRate | R
.7 | CurrentRSSI | WlanRSSI | R
.8 | CurrentRSSI1 | WlanRSSI | R
.9 | CurrentRSSI2 | WlanRSSI | R
.10 | CurrentRSSI3 | WlanRSSI | R
.11 | CurrentNoise | WlanRSSI | R
.12 | RxFrames54 | Counter32 | R
.13 | RxFrames48 | Counter32 | R
.14 | RxFrames36 | Counter32 | R
.15 | RxFrames24 | Counter32 | R
.16 | RxFrames18 | Counter32 | R
.17 | RxFrames12 | Counter32 | R
.18 | RxFrames11 | Counter32 | R
.19 | RxFrames9 | Counter32 | R
.20 | RxFrames6 | Counter32 | R
.21 | RxFrames5 | Counter32 | R
.22 | RxFrames2 | Counter32 | R
.23 | RxFrames1 | Counter32 | R
.24 | TxFrames54 | Counter32 | R
.25 | TxFrames48 | Counter32 | R
.26 | TxFrames36 | Counter32 | R
.27 | TxFrames24 | Counter32 | R
.28 | TxFrames18 | Counter32 | R
.29 | TxFrames12 | Counter32 | R
.30 | TxFrames11 | Counter32 | R
.31 | TxFrames9 | Counter32 | R
.32 | TxFrames6 | Counter32 | R
.33 | TxFrames5 | Counter32 | R
.34 | TxFrames2 | Counter32 | R
.35 | TxFrames1 | Counter32 | R
IfIndex
IfIndex of the WDS.
MSDUTx
This attribute counts the total number of packets transmitted on this WDS link.
MSDURx
This attribute counts the total number of packets received on this WDS link.
BytesTx
This attribute counts the total number of octets transmitted on this WDS link.
BytesRx
This attribute counts the total number of octets received on this WDS link.
CurrentRate
This attribute returns the current receive data rate for this link in 500 Kbps units, or 0 if no connection can be established.
CurrentRSSI
This attribute returns the current receive signal strength for this link, or 0 if no connection can be established.
CurrentRSSI1
This attribute returns the current receive signal strength on the first receiver for this link, or 0 if no connection can be established.
CurrentRSSI2
This attribute returns the current receive signal strength on the second receiver for this link, or 0 if no second receiver present or no connection can be established.
CurrentRSSI3
This attribute returns the current receive signal strength on the third receiver for this link, or 0 if no third receiver present or no connection can be established.
CurrentNoise
This attribute shows the measured noise level in dBm, or 0 if no connection can be established.
RxFrames54
This attribute shows the number of data frames that were received at 54 Mbps.
RxFrames48
This attribute shows the number of data frames that were received at 48 Mbps.
RxFrames36
This attribute shows the number of data frames that were received at 36 Mbps.
RxFrames24
This attribute shows the number of data frames that were received at 24 Mbps.
RxFrames18
This attribute shows the number of data frames that were received at 18 Mbps.
RxFrames12
This attribute shows the number of data frames that were received at 12 Mbps.
RxFrames11
This attribute shows the number of data frames that were received at 11 Mbps.
RxFrames9
This attribute shows the number of data frames that were received at 9 Mbps.
RxFrames6
This attribute shows the number of data frames that were received at 6 Mbps.
RxFrames5
This attribute shows the number of data frames that were received at 5.5 Mbps.
RxFrames2
This attribute shows the number of data frames that were received at 2 Mbps.
RxFrames1
This attribute shows the number of data frames that were received at 1 Mbps.
TxFrames54
This attribute shows the number of data frames that were transmitted at 54 Mbps.
TxFrames48
This attribute shows the number of data frames that were transmitted at 48 Mbps.
TxFrames36
This attribute shows the number of data frames that were transmitted at 36 Mbps.
TxFrames24
This attribute shows the number of data frames that were transmitted at 24 Mbps.
TxFrames18
This attribute shows the number of data frames that were transmitted at 18 Mbps.
TxFrames12
This attribute shows the number of data frames that were transmitted at 12 Mbps.
TxFrames11
This attribute shows the number of data frames that were transmitted at 11 Mbps.
TxFrames9
This attribute shows the number of data frames that were transmitted at 9 Mbps.
TxFrames6
This attribute shows the number of data frames that were transmitted at 6 Mbps.
TxFrames5
This attribute shows the number of data frames that were transmitted at 5.5 Mbps.
TxFrames2
This attribute shows the number of data frames that were transmitted at 2 Mbps.
TxFrames1
This attribute shows the number of data frames that were transmitted at 1 Mbps.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH