>> MIB - Management Information Base
>> Table: voipCallTable - (.1.3.6.1.4.1.272.4.33.3.1)
Description: Table of current VoIP calls (counterpart to isdnCallTable).
voipCallTable
OID | Name | Type | Access
.1 | TimeStamp | Date | R
.2 | ProtocolType | ENUM | R
.3 | State | ENUM | R
.4 | Role | ENUM | D
.5 | RefValue | INTEGER | R
.6 | Id | OCTET STRING | R
.7 | LocalNumber | DisplayString | R
.8 | LocalAlias | DisplayString | R
.9 | LocalIpAddr | IpAddress | R
.10 | LocalIpPort | INTEGER | R
.11 | RemoteNumber | DisplayString | R
.12 | RemoteAlias | DisplayString | R
.13 | RemoteIpAddr | IpAddress | R
.14 | RemoteIpPort | INTEGER | R
.15 | RemoteEndpointVendor | DisplayString | R
.16 | NegotiatedCodec | ENUM | R
.17 | TxPacketLengthMs | INTEGER | R
.18 | TxPackets | Counter32 | R
.19 | TxOctets | Counter32 | R
.20 | RxPacketLengthMs | INTEGER | R
.21 | RxPackets | Counter32 | R
.22 | RxOctets | Counter32 | R
.23 | DisconnectCause | DisplayString | R
.24 | Connect | INTEGER | R
.25 | If | INTEGER | R
TimeStamp
Timestamp of call (connection) establishment. Range: 0 to -1
ProtocolType
The VoIP protocol used for the active call. Enumerations: h323 (1) mgcp (2) sip (3) ipi (4)
State
Tracks the call state of the active call. Enumerations: admission (1) off-hook (2) dialing (3) called (4) proceeding (5) alerting (6) connected (7) disconnect (8) disengage (9) release (10) hold (11) conference (12) idle (13) transfer (14) overlapped (15)
Role
The endpoints role in the active call. Enumerations: caller (1) called (2) delete (3)
RefValue
Unique number which identifies the call (Q.931 compatible). Range: 0 to 32767
Id
Call-ID of the associated call.
LocalNumber
Internal number of local user. Length: 0 to 255
LocalAlias
Optional alias of local user. Length: 0 to 255
LocalIpAddr
IP address used by local user.
LocalIpPort
Associated port number used by local user. Range: 1 to 65535
RemoteNumber
Number of remote user if available. Length: 0 to 255
RemoteAlias
Alias of remote user if available. Length: 0 to 255
RemoteIpAddr
IP address used by remote user.
RemoteIpPort
Associated port number used by remote user. Range: 1 to 65535
RemoteEndpointVendor
Vendor's product description used by remote user. Length: 0 to 255
NegotiatedCodec
Used codec negotiated during connection establishment. Enumerations: g711a (1) g711u (2) g723-53 (3) g723-63 (4) g726-16 (5) g726-24 (6) g726-32 (7) g726-40 (8) g728 (9) g729 (10) g729a (11) g729b (12) t38udp (13) t38tcp (14) gsm (15) g722 (16) data (17) dtmf (18)
TxPacketLengthMs
Audio data length in milliseconds transmitted in a single frame. Range: 1 to 255
TxPackets
Number of RTP packets transmitted.
TxOctets
Number of octets transmitted.
RxPacketLengthMs
Audio data length in milliseconds received in a single frame. Range: 1 to 255
RxPackets
Number of RTP packets received.
RxOctets
Number of octets received.
DisconnectCause
Saves the disconnect reason of call after termination. Length: 0 to 255
Connect
Call connection time stamp (internal representation).
If
Index of interface for this call in case of protocol type ipi.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH