>> MIB - Management Information Base
>> Table: mpsReRouteApplTable - (.1.3.6.1.4.1.272.4.53.13.5.1)
Description: This table contains settings for the reroute application.
mpsReRouteApplTable
OID | Name | Type | Access
.1 | Index | ReRouteApplIndex | RW
.2 | Descr | DisplayString | RW
.3 | Type | ENUM | RW
.4 | Calendar | CalendarIndexOrZero | RW
.5 | AdminStatus | ENUM | D
Index
A unique value for each reroute application. Range: 1 to 65535
Descr
This variable contains the name of the rerouting application. Length: 0 to 32
Type
This variable contains type of the rerouting application. trunkNumber: used for external trunk numbers with call distribution 'reroute'. extension : used for internal extension numbers and individual rerouting. global : used for internal extension numbers and global rerouting. To use this, the flag 'use-global-rerouting' in mpsCoSFacilities(mpsClassOfServiceTable) must be active. Enumerations: trunkNumber (1) extension (2) global (3)
Calendar
Select a calendar index to switch the acitve mode this rerouting application automatically. Range: 0 to 65535
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH