>> MIB - Management Information Base
>> Table: ipSif - (.1.3.6.1.4.1.272.4.5.37)
ipSif
OID | Name | Type | Access
.1 | AdminStatus | ENUM | RW
.2 | LocalFilter | ENUM | RW
.3 | InterfaceFilter | ENUM | RW
.4 | Sysloglevel | ENUM | RW
.5 | UdpTimeout | INTEGER | RW
.6 | TcpTimeout | INTEGER | RW
.7 | PPTPTimeout | INTEGER | RW
.8 | DefaultTimeout | INTEGER | RW
.9 | MaxSessions | INTEGER | RW
.14 | MaxRejectEntries | INTEGER | RW
.15 | MaxRejectTtl | INTEGER | RW
.16 | InterfaceAliasAutoCreate | ENUM | RW
AdminStatus
Enable or disable Stateful Inspection Firewall. Enumerations: enable (1) disable (2)
LocalFilter
Enable or disable filtering on local requests Enumerations: enable (1) disable (2)
InterfaceFilter
Enable or disable filtering on same Interface packets Enumerations: enable (1) disable (2)
Sysloglevel
Levels for less or more Informations in the Syslog, verbose : display all Sif Activity deny : display only rejects, ignore accept : display only accpts none : disable Syslogs Enumerations: deny (1) accept (2) verbose (3) none (4)
UdpTimeout
Timeout on inactive UDP Session Range: 30 to 86400
TcpTimeout
Timeout on inactive TCP Session Range: 30 to 86400
PPTPTimeout
Timeout on inactive PPTP Session Range: 30 to 86400
DefaultTimeout
Timeout on all other ip Sessions Range: 30 to 86400
MaxSessions
Maximum number of monitored sessions Range: 0 to 1000000
MaxRejectEntries
Maximum number of ipSifRejectTable entries Range: 0 to 10000
MaxRejectTtl
Maximum time to live of the ipSifRejectTable entries in seconds Range: 5 to 86400
InterfaceAliasAutoCreate
Enable or disable automatic creation of interface aliases (see ipSifAliasAddressTable) due to created MPR interfaces visible in ifTable. Enumerations: enable (1) disable (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH