>> MIB - Management Information Base
>> Table: mpsTerminalCmdTable - (.1.3.6.1.4.1.272.4.53.14.4.1)
Description: The mpsTerminalCmdTable is used to trigger OpenStage provisioning actions at OpenStage phones. Creating entries: Entries are added to this table by assigning a value of the mpsTerminalCmd and mpsTerminalCmdMacAddress. Deleting Entries: Entries are removed by the ost application after the requested command has been performed and a new command for the same Teminal (same mpsTerminalCmdMacAddress) is present.
mpsTerminalCmdTable
OID | Name | Type | Access
.1 | MacAddress | MacAddress | RW
.2 | Cmd | ENUM | RW
.3 | State | ENUM | R
MacAddress
The MAC Address of the OpenStage Phone. Reference to mpsTerminalStatusTable MacAddress. Length: 6 to 6
Cmd
Command for configuration handling. Possible values are : none(1) -> default value fw-update(2) -> new firmware file shall be stored on the device reset-passwd(3) -> set admin password to default on the device. reset-upasswd(4) -> set user password to default on the device. Enumerations: none (1) fw-update (2) reset-passwd (3) reset-upasswd (4)
State
The state of this command (i.e., mpsTerminalStatusCmd). todo(1) : the command will start soon running(2) : the command is currently executing done(3) : the command has successfully completed error(4) : the command has failed Enumerations: todo (1) running (2) done (3) error (4)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH