>> MIB - Management Information Base
>> Table: gpsConfig - (.1.3.6.1.4.1.272.4.68.1)
gpsConfig
OID | Name | Type | Access
.1 | NMEATcpPort | INTEGER | RW
.2 | TimeUpdate | INTEGER | RW
.3 | OnlineMap | ENUM | RW
NMEATcpPort
This object represents the TCP port the NMEA data is exported to, use a value of -1 to disable exporting of NMEA data via TCP. Range: -1 to 65535
TimeUpdate
This object specifies interval for updating the system time via GPS time. -1 means don't use GPS time, 0 update on every GPS fix.
OnlineMap
This object enables or disables usgae of online maps in GUI. Enumerations: enabled (1) disabled (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH