>> MIB - Management Information Base
>> Table: dot11RSNAConfigTable - (.1.2.840.10036.1.9.1)
Description: An entry in the dot11RSNAConfigTable.
dot11RSNAConfigTable
OID | Name | Type | Access
.2 | ConfigVersion | Integer32 | R
.3 | ConfigPairwiseKeysSupported | Unsigned32 | R
.4 | ConfigGroupCipher | OCTET STRING | RW
.5 | ConfigGroupRekeyMethod | ENUM | RW
.6 | ConfigGroupRekeyTime | Unsigned32 | RW
.7 | ConfigGroupRekeyPackets | Unsigned32 | RW
.8 | ConfigGroupRekeyStrict | ENUM | RW
.9 | ConfigPSKValue | OCTET STRING | RW
.10 | ConfigPSKPassPhrase | DisplayString | RW
.13 | ConfigGroupUpdateCount | Unsigned32 | RW
.14 | ConfigPairwiseUpdateCount | Unsigned32 | RW
.15 | ConfigGroupCipherSize | Unsigned32 | R
.16 | ConfigPMKLifetime | Unsigned32 | RW
.17 | ConfigPMKReauthThreshold | Unsigned32 | RW
.18 | ConfigNumberOfPTKSAReplayCounters | INTEGER | R
.19 | ConfigSATimeout | Unsigned32 | RW
.20 | AuthenticationSuiteSelected | OCTET STRING | R
.21 | PairwiseCipherSelected | OCTET STRING | R
.22 | GroupCipherSelected | OCTET STRING | R
.23 | PMKIDUsed | OCTET STRING | R
.24 | AuthenticationSuiteRequested | OCTET STRING | R
.25 | PairwiseCipherRequested | OCTET STRING | R
.26 | GroupCipherRequested | OCTET STRING | R
.27 | TKIPCounterMeasuresInvoked | Unsigned32 | RW
.28 | 4WayHandshakeFailures | Unsigned32 | RW
.29 | ConfigNumberOfGTKSAReplayCounters | INTEGER | R
ConfigVersion
The highest RSNA version this entity supports. See 7.3.2.9.
ConfigPairwiseKeysSupported
This object indicates how many pairwise keys the entity supports for RSNA.
ConfigGroupCipher
This object indicates the group cipher suite selector the entity must use. The group cipher suite in the RSN Information Element shall take its value from this variable. It consists of an OUI (the first 3 octets) and a cipher suite identifier (the last octet). Length: 4 to 4
ConfigGroupRekeyMethod
This object selects a mechanism for rekeying the RSNA GTK. The default is time-based, once per day. Rekeying the GTK is only applicable to an entity acting in the Authenticator role (an AP in an ESS). Enumerations: disabled (1) timeBased (2) packetBased (3) timepacket-Based (4)
ConfigGroupRekeyTime
The time in seconds after which the RSNA GTK shall be refreshed. The timer shall start at the moment the GTK was set using the MLMESETKEYS. request primitive. Range: 1 to -1
ConfigGroupRekeyPackets
A packet count (in 1000s of packets) after which the RSNA GTK shall be refreshed. The packet counter shall start at the moment the GTK was set using the MLME-SETKEYS.request primitive and it shall count all packets encrypted using the current GTK. Range: 1 to -1
ConfigGroupRekeyStrict
This object signals that the GTK shall be refreshed whenever a STA leaves the BSS that possesses the GTK. Enumerations: true (1) false (2)
ConfigPSKValue
The PSK for when RSNA in PSK mode is the selected AKM suite. In that case, the PMK will obtain its value from this object. This object is logically write-only. Reading this variable shall return unsuccessful status or null or zero. Length: 32 to 32
ConfigPSKPassPhrase
The PSK, for when RSNA in PSK mode is the selected AKM suite, is configured by dot11RSNAConfigPSKValue. An alternative manner of setting the PSK uses the password-to-key algorithm defined in H.4. This variable provides a means to enter a pass-phrase. When this object is written, the RSNA entity shall use the password-to-key algorithm specified in H.4 to derive a preshared and populate dot11RSNAConfigPSKValue with this key. This object is logically write-only. Reading this variable shall return unsuccessful status or null or zero. Length: 0 to 255
ConfigGroupUpdateCount
The number of times Message 1 in the RSNA Group Key Handshake will be retried per GTK Handshake attempt. Range: 1 to -1
ConfigPairwiseUpdateCount
The number of times Message 1 and Message 3 in the RSNA 4-Way Handshake will be retried per 4-Way Handshake attempt. Range: 1 to -1
ConfigGroupCipherSize
This object indicates the length in bits of the group cipher key. Range: 0 to -1
ConfigPMKLifetime
The maximum lifetime of a PMK in the PMK cache. Range: 1 to -1
ConfigPMKReauthThreshold
The percentage of the PMK lifetime that should expire before an IEEE 802.1X reauthentication occurs. Range: 1 to 100
ConfigNumberOfPTKSAReplayCounters
Specifies the number of PTKSA replay counters per association: 0 -> 1 replay counter, 1 -> 2 replay counters, 2 -> 4 replay counters, 3 -> 16 replay counters
ConfigSATimeout
The maximum time a security association shall take to set up. Range: 1 to -1
AuthenticationSuiteSelected
The selector of the last AKM suite negotiated. Length: 4 to 4
PairwiseCipherSelected
The selector of the last pairwise cipher negotiated. Length: 4 to 4
GroupCipherSelected
The selector of the last group cipher negotiated. Length: 4 to 4
PMKIDUsed
The selector of the last PMKID used in the last 4-Way Handshake. Length: 16 to 16
AuthenticationSuiteRequested
The selector of the last AKM suite requested. Length: 4 to 4
PairwiseCipherRequested
The selector of the last pairwise cipher requested. Length: 4 to 4
GroupCipherRequested
The selector of the last group cipher requested. Length: 4 to 4
TKIPCounterMeasuresInvoked
Counts the number of times that a TKIP MIC failure occurred two times within 60 s and TKIP countermeasures were invoked. This attribute counts both local and remote MIC failure events reported to this STA. It increments every time TKIP countermeasures are invoked Range: 1 to -1
4WayHandshakeFailures
Counts the number of 4-Way Handshake failures. Range: 1 to -1
ConfigNumberOfGTKSAReplayCounters
Specifies the number of GTKSA replay counters per association: 0 -> 1 replay counter, 1 -> 2 replay counters, 2 -> 4 replay counters, 3 -> 16 replay counters

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH