>> MIB - Management Information Base
>> Table: igmpInterfaceOperTable - (.1.3.6.1.4.1.272.4.5.51.8.1)
Description: An entry (conceptual row) representing an interface on which IGMP is currently operating.
igmpInterfaceOperTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | R
.2 | QueryInterval | Unsigned32 | R
.4 | Version | Unsigned32 | R
.5 | Querier | IpAddress | R
.6 | QueryMaxResponseTime | Unsigned32 | R
.7 | QuerierUpTime | TimeTicks | R
.8 | QuerierExpiryTime | TimeTicks | R
.9 | Version1QuerierTimer | TimeTicks | R
.10 | WrongVersionQueries | Counter32 | R
.11 | Joins | Counter32 | R
.12 | ProxyIfIndex | InterfaceIndexOrZero | R
.13 | Groups | Gauge32 | R
.14 | Robustness | Unsigned32 | R
.15 | LastMembQueryIntvl | Unsigned32 | R
.16 | Version2QuerierTimer | TimeTicks | R
.17 | GeneralQueryTimer | TimeTicks | R
.18 | StateLimit | Unsigned32 | R
.19 | HostOnlyMode | ENUM | R
IfIndex
The ifIndex value of the interface for which IGMP is operating. Range: 1 to 2147483647
QueryInterval
The frequency at which IGMP Host-Query packets are transmitted on this interface.
Version
The version of IGMP which is running on this interface.
Querier
The address of the IGMP Querier on the IP subnet to which this interface is attached.
QueryMaxResponseTime
The maximum query response time advertised in IGMPv2 queries on this interface. Range: 0 to 255
QuerierUpTime
The time since igmpInterfaceOperQuerier was last changed.
QuerierExpiryTime
The time when the Other Querier Present Timer expires. If the local system is the querier, the value of this object is zero.
Version1QuerierTimer
The time when the host assumes that there are no IGMPv1 routers present on the interface. While this is non- zero, the host will reply to all queries with version 1 membership reports.
WrongVersionQueries
The number of queries received whose IGMP version does not match igmpInterfaceOperVersion, over the lifetime of the row entry. IGMP requires that all routers on a LAN be configured to run the same version of IGMP. Thus, if any queries are received with the wrong version, this indicates a configuration error.
Joins
The number of times a group membership has been added on this interface; that is, the number of times an entry for this interface has been added to the Cache Table. This object gives an indication of the amount of IGMP activity over the lifetime of the row entry.
ProxyIfIndex
Some devices implement a form of IGMP proxying whereby memberships learned on the interface represented by this row, cause IGMP Host Membership Reports to be sent on the interface whose ifIndex value is given by this object. Such a device would implement the igmpV2RouterMIBGroup only on its router interfaces (those interfaces with non-zero igmpInterfaceOperProxyIfIndex). Typically, the value of this object is 0, indicating that no proxying is being done. Range: 0 to 2147483647
Groups
The current number of entries for this interface in the Cache Table.
Robustness
The Robustness Variable allows tuning for the expected packet loss on a subnet. If a subnet is expected to be lossy, the Robustness Variable may be increased. IGMP is robust to (Robustness Variable-1) packet losses. Range: 1 to 255
LastMembQueryIntvl
The Last Member Query Interval is the Max Response Time inserted into Group-Specific Queries sent in response to Leave Group messages, and is also the amount of time between Group-Specific Query messages. This value may be tuned to modify the leave latency of the network. A reduced value results in reduced time to detect the loss of the last member of a group. The value of this object is irrelevant if igmpInterfaceOperVersion is 1. Range: 0 to 255
Version2QuerierTimer
The time when the host assumes that there are no IGMPv2 routers present on the interface. While this is non- zero, the host will reply to all queries with version 1 or 2 membership reports.
GeneralQueryTimer
The time when the next general Query is issued on this interface.
StateLimit
The maximum allowed number of Reports/Queries per seconds on this interface. Must be greater zero to be active.
HostOnlyMode
An indication of whether the interface is running in host-only mode. If set to false this interface will operate in host and routing mode. Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH