>> MIB - Management Information Base
>> Table: tr069IpLANDeviceXrefTable - (.1.3.6.1.4.1.272.4.22.6.2.11.1)
Description: An entry containing a cross reference between an IPInterface object and associated local table entries.
tr069IpLANDeviceXrefTable
OID | Name | Type | Access
.1 | DeviceIdx | INTEGER | RW
.2 | IpInterfaceIdx | INTEGER | RW
.3 | HostCfgIfIndex | INTEGER | RW
.4 | Type | ENUM | D
.5 | Address | IpAddress | RW
.6 | Mask | IpAddress | RW
.7 | Enable | ENUM | RW
.8 | XMLTreeState | ENUM | RW
DeviceIdx
Index of the LANDevice associated with this entry as presented to TR-069. Range: 0 to 2147483647
IpInterfaceIdx
Index of this IpInterface as presented to TR-069. Range: 1 to 2147483647
HostCfgIfIndex
Identifier representing the interface that carries the IP configuration associated with this entry.
Type
Addressing type of this interface. Enumerations: dhcp (1) static (2) delete (3)
Address
IP address associated with this entry. Has no effect if Type == dhcp.
Mask
Netmask associated with this entry. Has no effect if Type == dhcp.
Enable
Whether this entry is enabled. Enumerations: false (1) true (2)
XMLTreeState
Whether this entry is present in the XML tree. Enumerations: setup (1) new (2) present (3) purge (4)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH