>> MIB - Management Information Base
>> Table: systemPhoneAudioTable - (.1.3.6.1.4.1.272.4.64.1.2.1)
Description: This table contains information about audio settings of system phones. An entry in this table will also be deleted if the related systemPhoneTable entry is deleted.
systemPhoneAudioTable
OID | Name | Type | Access
.1 | Index | SystelTerminalIndex | RW
.2 | Fac | BITS | RW
.3 | HeadsetType | INTEGER | RW
.4 | VolSpeaker | SystelAudioVolume | RW
.5 | VolHandset | INTEGER | RW
.6 | VolCallWaitingBeep | SystelAudioVolume | RW
.7 | VolDoNotDisturbBeep | SystelAudioVolume | RW
.8 | VolAppointedTimeBeep | INTEGER | RW
.9 | VolNotifyBeep | INTEGER | RW
.10 | VolAnswMachOKBeep | INTEGER | RW
.11 | AdminStatus | ENUM | D
.12 | NGVolHeadset | SystelAudioVolume | RW
.13 | NGVolAcknowledgeBeep | SystelAudioVolume | RW
.14 | NGMicHeadsetResp | INTEGER | RW
Index
Reference to the mpsTerminalTable. Range: 1 to 65535
Fac
Facility settings for audio control: out-ringing : Normal ringing tones can be heard on the internal speaker [0] or on the internal speaker and an additional speaker connected to 'audio out' [1]. out-paging : Incomming announcements can be heard on the internal speaker [0] or on the internal speaker and an additional speaker connected to 'audio out' [1]. out-listening : Hands-free listening can be heard on the internal speaker [0] or on the internal speaker and an additional speaker connected to 'audio out' [1]. out-handsfree : Hands-free talking and system call exchange can be heard on the internal speaker [0] or on the internal speaker and an additional speaker connected to 'audio out' [1]. out-answ-mach : Call of messages of anwering machine can be heard on the internal speaker [0] or on the internal speaker and an additional speaker connected to 'audio out' [1]. headset : Setting this bit to [1] enables some automatic headset functions: --> if function keys auto call acceptance AND headset are adjusted AND the user activates the auto call acceptance function key, the headset automatically answer the call --> furthermore, if function keys trunk-line key OR extension key adjusted, pressing such a keys leads to automatically calling via headset handsfree-mute : Enable [1] or disbable [0] mute after handsfree calling. beep-negative-ack : Enable [1] or disbable [0] negative ack beep tone. beep-positive-ack : Enable [1] or disbable [0] positive ack beep tone. beep-call-waiting-repeat : Setting this bit to [0] means that the user is noticed onced. Setting this bit to [1], causes beep-tone of call waiting signal to be repeated. Enumerations: out-ringing (0) out-paging (1) out-listening (2) out-handsfree (3) out-answ-mach (4) headset (5) handsfree-mute (6) beep-negative-ack (7) beep-positive-ack (8) beep-call-waiting-repeat (9)
HeadsetType
The headset type. Value currently only used within the system phone, but must be saved in the PBX. Range: 0 to 255
VolSpeaker
Specifies volume setting for telephone speaker. For NG phones range was changed (0 .. 10). Range: 0 to 10
VolHandset
Specifies volume setting for telephone handset. Range: 0 to 3
VolCallWaitingBeep
Specifies volume setting for call waiting tone. For NG phones range was changed (0 .. 10). Range: 0 to 10
VolDoNotDisturbBeep
Specifies volume setting for do not disturb tone. For NG phones range was changed (0 .. 10). Range: 0 to 10
VolAppointedTimeBeep
Specifies volume setting for appointed time call tone. Range: 0 to 6
VolNotifyBeep
Specifies volume setting for notify beep tone. Range: 0 to 2
VolAnswMachOKBeep
Specifies volume setting for answering machine acknowledgement tone. Range: 0 to 2
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
NGVolHeadset
Specifies volume setting for headset. This mib item is only important for NG phones. Range: 0 to 10
NGVolAcknowledgeBeep
Specifies volume setting for acknowledgement beep tone. This mib item is only important for NG phones. Range: 0 to 10
NGMicHeadsetResp
Specifies responsivity settings for microphone of headset. This mib item is only important for NG phones. Range: 1 to 3

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH