>> MIB - Management Information Base
>> Table: pptpProfileTable - (.1.3.6.1.4.1.272.4.23.1.1)
Description: The pptpProfileTable contains parameters for the Point-to-Point Tunneling Protocol (PPTP) according RFC 2637. Entries are removed by setting an entry's pptpProfileKeepalive object to 'delete'.
pptpProfileTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | Keepalive | ENUM | D
.3 | MaxRequests | INTEGER | RW
.4 | MaxBlockTime | INTEGER | RW
.5 | MaxAckTimeout | INTEGER | RW
.6 | ReassemblyTimeout | INTEGER | RW
.7 | MaxSWin | INTEGER | RW
.8 | XmitWaitTime | INTEGER | RW
.9 | MaxCtlConn | INTEGER | RW
.10 | GreWindowAdaption | ENUM | RW
.11 | Host | DisplayString | RW
.12 | Vendor | DisplayString | RW
.13 | FirmRev | INTEGER | RW
Id
The profile ID of the PPTP profile.
Keepalive
When set to on(1), PPTP echo requests as described in RFC 2637 are sent in regular intervals during the connection. If set to off(2), no PPTP echo requests will be performed, delete(3) determines the entry is marked for discard. Enumerations: on (1) off (2) delete (3)
MaxRequests
The maximum number of outstanding PPTP echo replies, until the PPTP control connection is droped and all associated calls are terminated. Range: 0 to 100
MaxBlockTime
Maximum time (in msec) the GRE Send Window is blocked. If the GRE Send Window is full, no packets can be forwarded and the Maximum Time is passed, the GRE Send Window is resetted to prevent unsolvable situations. Range: 0 to 10000
MaxAckTimeout
Maximum value the adaptive Acknowledgment Timeout (in msec) can reach while it is calculated. According to RFC 2637. Range: 2000 to 5000
ReassemblyTimeout
Maximum time (in msec) for rearranging out-of-sequence packets. After this time outstanding packets will be supposed missing. Range: 100 to 1000
MaxSWin
Maximum GRE send window size Range: 0 to 256
XmitWaitTime
Wait time (in msec) before transmitting data. Range: 0 to 32
MaxCtlConn
Defines the maximum number of incoming PPTP control connections per remote IP address. Range: 1 to 1024
GreWindowAdaption
Enables/disables the sliding GRE window algorithm. Enumerations: enabled (1) disabled (2)
Host
Specific name of the PAC or PNS being used for the PPTP Start Control Connection Request/Reply. Length: 0 to 255
Vendor
Vendor specific string describing the type of PAC or PNS being used for the PPTP Start Control Connection Request/Reply. Length: 0 to 255
FirmRev
This variable contains the firmware revision number of the issuing PAC or PNS. If not specified (set to 0) the global Firmware Revision will be propagated. Range: -1 to 999

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH