>> MIB - Management Information Base
>> Table: ipRipTimerTable - (.1.3.6.1.4.1.272.4.5.23.1)
Description: The 'ipRipTimerTable' contains the basic configuration of the RIP protocol. Formerly created to define only the 3 timers involved in RIP process (cf RFC 2453). This set of timers is unique for the router. Values should be the same on all the routers of the whole network.
ipRipTimerTable
OID | Name | Type | Access
.1 | Version | INTEGER | R
.2 | TimerUpdate | INTEGER | RW
.3 | TimerTimeout | INTEGER | RW
.4 | TimerGarbage | INTEGER | RW
.5 | Rfc2453Timer | ENUM | RW
.6 | Rfc2091Timer | ENUM | RW
.7 | UpdatePacketRetryTimer | INTEGER | RW
.8 | PoisonedReverse | ENUM | RW
.9 | DistributeDefaultRoutes | ENUM | RW
.10 | HoldDownTimer | INTEGER | RW
Version
RFC 2453, RIP Version 2. Range: 1 to 3
TimerUpdate
An unsollicited RIP response is broadcast every 'ipRipTimerUpdate' seconds. Range: 1 to 65535
TimerTimeout
If 'ipRipTimerTimeout' seconds elapse from the last time an update message is received for this route, the route is dropped but keeped in routing table. Then 'garbage process' is started. Range: 1 to 65535
TimerGarbage
If 'ipRipTimerGarbage' seconds elapse from the start of 'garbage process' (and if route is still 'dropped'), the route is removed from the routing table. Range: 1 to 65535
Rfc2453Timer
The 'ipRipRfc2453Timer' enabled/disables variable timer definition from RFC 2453. Enumerations: enabled (1) disabled (2)
Rfc2091Timer
The 'ipRipRfc2453Timer' enabled/disables variable timer definition from RFC 2091. Enumerations: enabled (1) disabled (2)
UpdatePacketRetryTimer
If 'ipRipTimerUpdatePacketRetry' seconds elapse since the transmission of the last update packet without receiving an acknowledge the update packet is resend. Range: 1 to 10
PoisonedReverse
Enable or disable the (currently unimplemented) control over 'poisoned reverse' route distribution. Enumerations: enabled (1) disabled (2)
DistributeDefaultRoutes
Enable or disable the distribution of 'default routes'. Enumerations: enabled (1) disabled (2)
HoldDownTimer
If 'ipRipHoldDownTimer' seconds elapse from the start of 'database timeout' (and if route is still 'dropped'), the route is removed from the routing table. Range: 1 to 65535

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH