>> MIB - Management Information Base
>> Table: ospfStubAreaTable - (.1.3.6.1.2.1.14.3.1)
Description: The metric for a given Type of Service that will be advertised by a default Area Border Router into a stub area.
ospfStubAreaTable
OID | Name | Type | Access
.1 | AreaId | IpAddress | RW
.2 | TOS | INTEGER | R
.3 | Metric | INTEGER | RW
.4 | Status | ENUM | D
.5 | MetricType | ENUM | RW
AreaId
The 32 bit identifier for the Stub Area. On creation, this can be derived from the instance.
TOS
The Type of Service associated with the metric. On creation, this can be derived from the instance. Range: 0 to 31
Metric
The metric value applied at the indicated type of service. By default, this equals the least metric at the type of service among the interfaces to other areas. Range: 1 to 16777215
Status
This variable displays the validity or invalidity of the entry. Setting it to 'invalid' has the effect of rendering it inoperative. The internal effect (row removal) is implementation dependent. Enumerations: valid (1) invalid (2)
MetricType
This variable displays the type of metric ad- vertised as a default route. Enumerations: ospfMetric (1) comparableCost (2) nonComparable (3)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH