>> MIB - Management Information Base
>> Table: hwAccelChanCapTable - (.1.3.6.1.4.1.272.4.63.1.2.1)
Description: This object contains a HW accelerator channel capability.
hwAccelChanCapTable
OID | Name | Type | Access
.1 | Slot | INTEGER | R
.2 | Unit | INTEGER | R
.3 | Chan | INTEGER | R
.4 | Capability | ENUM | R
.5 | MinKeySize | INTEGER | R
.6 | MaxKeySize | INTEGER | R
Slot
The slot number of this HW accelerator channel.
Unit
The unit number of this HW accelerator channel.
Chan
The channel number of this HW accelerator channel.
Capability
The supported capability of this HW accelerator. Enumerations: des-cbc (1) des3-cbc (2) aes-cbc (3) rc4 (4) md5 (5) sha1 (6) rsa (7) rng (8)
MinKeySize
This object specifies the minimum key or field size used with this capability. A key size of 0 means that a explicity key size is not applicable. Range: 0 to 2560
MaxKeySize
This object specifies the maximum key or field size used with this capability. A key size of 0 means that a explicity key size is not applicable. Range: 0 to 2560

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH