>> MIB - Management Information Base
>> Table: snmpAdmin - (.1.3.6.1.4.1.272.4.22.3.1)
snmpAdmin
OID | Name | Type | Access
.1 | Version | BITS | RW
.2 | Port | INTEGER | RW
.3 | TrapPort | INTEGER | RW
.4 | TrapCommunity | DisplayString | RW
.5 | TrapBrdCast | ENUM | RW
.6 | PrivIndex | ENUM | RW
.7 | GetOrder | ENUM | RW
.8 | LinkTrapEvent | ENUM | RW
.9 | McDiscovery | ENUM | RW
Version
This bitfield enables the active SNMP versions: v1 : SNMP V1 v2c : SNMP V2c (community, like v1 but with Counter64) v3 : SNMP V3 . Enumerations: v1 (0) v2c (1) v3 (2)
Port
SNMP listen port. Range: 0 to 65535
TrapPort
SNMP trap port. Range: 0 to 65535
TrapCommunity
Community name for sending traps. Length: 0 to 255
TrapBrdCast
Enable/disable trap broadcasting. Enumerations: on (1) off (2)
PrivIndex
This enables or disables the handling of the private OID part (.i): auto : the private OID part is appended automatically - depending on community name the private OID part is appended, if: - the community is appended with '+i' or with '' the private OID part is not appended, if: - the community is appended with '-i' the default is to append the private OID index auto_nopriv: the private OID part is appended automatically like 'auto', but the default is not to add the index both auto settings consider special marked tables (STDINDEX, EXTINDEX) always : the private OID part is always appended (this was the default on former version) never : the private OID part is never appended Usually the OIDs have the format: .1.3.6.x.x .y.y .i .1.3.6.x.x: is the constant part of the OID of the variable specified in MIB-source .y.y : is the specific part of the OID to identify exactly a row. It is the content of all index variables. .i : is a consecutively incremented index number, to distinguish rows with identical index variables Enumerations: auto (1) auto-nopriv (2) always (3) never (4)
GetOrder
This the handling of the private OID part (.i): normal : the GetNext returns the next object like stored in internal database. sorted : the GetNext return the next object sorted according to the index values (RFC-1157) Enumerations: normal (1) sorted (2)
LinkTrapEvent
Defines the ifOperStatus transition(s) of an ifTable object that generates a SNMP linkUp/linkDown trap: none : disable linkUp/linkDown trap generation. any : enable bintec like trap generation. - entering the up state generates a up trap - any other state change generates a down trap up : enable rfc1157 like trap generation. - entering the up state generates a up trap - leaving the up state generates a down trap down : enable rfc2233 like trap generation. - leaving the down state generates a up trap - entering the down state generates a down trap Seven parameters are sent in each linkUp/linkDown trap pdu: 1. ifEntry.ifIndex (mandatory for linkUp/Down traps) 2. ifEntry.ifDescr 3. ifEntry.ifType 4. ifEntry.ifAdminStatus 5. ifEntry.ifOperStatus 6. system.Description 7. system.Name Enumerations: none (1) any (2) up (3) down (4)
McDiscovery
Defines whether Multicast SNMP discovery is enabled or not. Enumerations: enabled (1) disabled (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH