>> MIB - Management Information Base
>> Table: layer2BridgeTable - (.1.3.6.1.4.1.272.4.56.1.1)
Description: Each entry consists of a unique MAC address and corresponding layer-2 informations.
layer2BridgeTable
OID | Name | Type | Access
.1 | MacAddr | MacAddress | R
.2 | PortIfIndex | INTEGER | R
.3 | LinkIfIndex | INTEGER | R
MacAddr
The MAC address identifying the host on layer-2. Length: 6 to 6
PortIfIndex
The layer-2 port over which the host is currently reachable.
LinkIfIndex
The bridge group the host logically belongs to.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH