>> MIB - Management Information Base
>> Table: wlcVSSStatTable - (.1.3.6.1.4.1.272.4.61.1.26.1)
Description: This table contains statistic information about each VSS.
wlcVSSStatTable
OID | Name | Type | Access
.1 | VSSIndex | INTEGER | R
.2 | Current | INTEGER | R
.3 | BytesTx | Counter32 | R
.4 | BytesRx | Counter32 | R
.5 | BSSID | MacAddress | R
.6 | OperState | ENUM | R
.7 | SoftTotalDenied | INTEGER | R
.8 | BSMovements | INTEGER | R
.9 | ClearCounter | ENUM | RW
.10 | TotalDenied | INTEGER | R
VSSIndex
The unique VSS index.
Current
Number of currently associated stations.
BytesTx
Transmitted Bytes.
BytesRx
Received Bytes.
BSSID
This object contains the current BSSID for the service set. Length: 6 to 6
OperState
This object contains the current OperState for the service set. Enumerations: true (1) false (2)
SoftTotalDenied
Number of rejected clients due to wlcVSSProfileSoftTotal limit.
BSMovements
Number of clients moved to other band by band steering mechanism.
ClearCounter
counting := accounting is active, clearing := clear all statistics Enumerations: counting (1) clearing (2)
TotalDenied
Number of rejected clients due to wlcVSSProfileTotal limit.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH