>> MIB - Management Information Base
>> Table: pppoaCallTable - (.1.3.6.1.4.1.272.4.28.1.1)
Description: The pppoaCallTable displays all currently active PPPoA calls. Only the system can add or remove entries to this table.
pppoaCallTable
OID | Name | Type | Access
.1 | Id | INTEGER | R
.2 | State | ENUM | RW
.3 | ReceivedPackets | Counter | R
.4 | ReceivedOctets | Counter | R
.5 | ReceivedErrors | Counter | R
.6 | TransmitPackets | Counter | R
.7 | TransmitOctets | Counter | R
.8 | TransmitErrors | Counter | R
.9 | Info | DisplayString | R
Id
Identification of the PPPoA call.
State
The state of the PPPoA discovery stage. Enumerations: idle (1) established (2) terminated (3)
ReceivedPackets
Count of received valid packets.
ReceivedOctets
Count of received valid Octets.
ReceivedErrors
Count of received invalid packets.
TransmitPackets
Count of transmitted packets.
TransmitOctets
Count of transmitted Octets.
TransmitErrors
Count of transmit errors.
Info
Additional information to identify the PPPoA call Length: 0 to 255

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH