>> MIB - Management Information Base
>> Table: sysPedRelay - (.1.3.6.1.4.1.272.4.17.6.1)
sysPedRelay
OID | Name | Type | Access
.1 | 1State | ENUM | RW
.2 | 2State | ENUM | RW
.31 | Count | INTEGER | R
1State
Relay control. open : Relay is open. closed: Relay is closed. Default state is open. Enumerations: open (1) closed (2)
2State
Relay control. open : Relay is open. closed: Relay is closed. Default state is open. Enumerations: open (1) closed (2)
Count
Number of available relays in the system.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH