>> MIB - Management Information Base
>> Table: wlcStationTable - (.1.3.6.1.4.1.272.4.61.1.28.1)
Description: The wlcStationTable contains information relating to the clients currently associated to our WTPs. Each entry corresponds to an associated client station (STA). Entries cannot be added or deleted by the user.
wlcStationTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | VSSIndex | INTEGER | R
.3 | Address | MacAddress | R
.4 | InetAddressType | ENUM | R
.5 | InetAddress | IpAddress | R
.6 | State | ENUM | D
.7 | Security | ENUM | R
.8 | MSDUTx | Counter32 | R
.9 | MSDURx | Counter32 | R
.10 | BytesTx | Counter32 | R
.11 | BytesRx | Counter32 | R
.12 | Rate | WlanRate | R
.13 | Signal | WlanRSSI | R
.14 | RSSI1 | WlanRSSI | R
.15 | RSSI2 | WlanRSSI | R
.16 | RSSI3 | WlanRSSI | R
.17 | Noise | WlanRSSI | R
.18 | UpTime | Counter32 | R
.19 | RxBW40 | ENUM | R
.20 | RxShortGI | ENUM | R
.21 | TxBW40 | ENUM | R
.22 | TxShortGI | ENUM | R
.23 | TxFrames11 | Counter32 | R
.24 | TxFrames24 | Counter32 | R
.25 | TxFrames54 | Counter32 | R
.26 | TxFramesMCS3 | Counter32 | R
.27 | TxFramesMCS7 | Counter32 | R
.28 | TxFramesMCS11 | Counter32 | R
.29 | TxFramesMCS15 | Counter32 | R
.30 | RxFrames11 | Counter32 | R
.31 | RxFrames24 | Counter32 | R
.32 | RxFrames54 | Counter32 | R
.33 | RxFramesMCS3 | Counter32 | R
.34 | RxFramesMCS7 | Counter32 | R
.35 | RxFramesMCS11 | Counter32 | R
.36 | RxFramesMCS15 | Counter32 | R
.37 | RxAirtime | Counter64 | R
.38 | TxAirtime | Counter64 | R
.39 | LastSeen | Date | R
.40 | RxDiscards | Counter32 | R
.41 | TxDiscards | Counter32 | R
Index
Unique station index.
VSSIndex
The interface index of the associated Service Set.
Address
MAC Address of the Assigned STA. Length: 6 to 6
InetAddressType
The IP address type of the STA. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
InetAddress
This attribute shows the IP address of the client. It is only available if any IP frames have been received from the client.
State
The current state of the station. Enumerations: none (1) associating (2) associated (3) authenticate (4) authenticated (5) delete (8)
Security
The Security Option of the Station. Enumerations: none (1) wep40 (2) wep104 (3) wpa-psk (4) wpa (5) wpa2 (6)
MSDUTx
This attribute counts the total number of packets transmitted to this station.
MSDURx
This attribute counts the total number of packets received from this station.
BytesTx
This attribute counts the total number of octets transmitted to this station.
BytesRx
This attribute counts the total number of octets received from this station.
Rate
This attribute reflects the data rate of the latest packet received from this station, in 500 kbps units. Range: 0 to 600
Signal
This attribute shows the received signal strength in dBm. Range: -110 to 0
RSSI1
This attribute shows the received signal strength at the first receiver in dBm. The value 0 indicates no connection. Range: -110 to 0
RSSI2
This attribute shows the received signal strength at the second receiver in dBm. The value 0 indicates no connection or no second receiver present. Range: -110 to 0
RSSI3
This attribute shows the received signal strength at the third receiver in dBm. The value 0 indicates no connection or no third receiver present. Range: -110 to 0
Noise
This attribute shows the measured noise level in dBm, or 0 if no connection can be established. Range: -110 to 0
UpTime
This attribute records the system uptime at the moment the client successfully finished association.
RxBW40
This attribute shows if the station is able to receive pakets with 40MHz bandwidth. Enumerations: true (1) false (2)
RxShortGI
This attribute shows if the station is able to receive pakets with short guard interval. Enumerations: true (1) false (2)
TxBW40
This attribute shows if the station is able to transmit pakets with 40 MHz bandwidth. Enumerations: true (1) false (2)
TxShortGI
This attribute shows if the station is able to transmit pakets with short guard interval. Enumerations: true (1) false (2)
TxFrames11
This attribute shows the number of data frames that were transmitted at 11 Mbps.
TxFrames24
This attribute shows the number of data frames that were transmitted at 24 Mbps.
TxFrames54
This attribute shows the number of data frames that were transmitted at 54 Mbps.
TxFramesMCS3
This attribute shows the number of HT data frames that were transmitted at MCS 3.
TxFramesMCS7
This attribute shows the number of HT data frames that were transmitted at MCS 7.
TxFramesMCS11
This attribute shows the number of HT data frames that were transmitted at MCS 11.
TxFramesMCS15
This attribute shows the number of HT data frames that were transmitted at MCS 15.
RxFrames11
This attribute shows the number of data frames that were received at 11 Mbps.
RxFrames24
This attribute shows the number of data frames that were received at 24 Mbps.
RxFrames54
This attribute shows the number of data frames that were received at 54 Mbps.
RxFramesMCS3
This attribute shows the number of HT data frames that were received at MCS 3.
RxFramesMCS7
This attribute shows the number of HT data frames that were received at MCS 7.
RxFramesMCS11
This attribute shows the number of HT data frames that were received at MCS 11.
RxFramesMCS15
This attribute shows the number of HT data frames that were received at MCS 15.
RxAirtime
Accumulated estimated time in microseconds for all unidirectional frames received from this station.
TxAirtime
Accumulated estimated time in microseconds for all unidirectional frames transmitted to this station.
LastSeen
Timestamp of the last received frame by this Station Range: 0 to -1
RxDiscards
Count of discarded bytes due to bandwidth limitation.
TxDiscards
Count of discarded bytes due to bandwidth limitation.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH