>> MIB - Management Information Base
>> Table: x25MprTable - (.1.3.6.1.4.1.272.4.6.7.1)
Description: This table contains an entry for each partner reachable via X.25 for Multiprotocol over X.25 according to RFC 1356. Entries in this table are created manually and will result to the creation of a multiprotocol routing interface in the ifTable. This interface can than be used by higher level protocols like ip, ipx and bridging. The object x25MprIfIndex shall be set to 0 for creation of new entries. The BRICK will allocate the next free interface index and assign it ti x25MprIfIndex. Rows of this table can be deleted by setting the object x25MprEncapsulation to the value delete.
x25MprTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RW
.2 | Mtu | INTEGER | RW
.3 | Encapsulation | ENUM | D
.4 | NumVC | INTEGER | RW
.5 | MaxVC | INTEGER | RW
.6 | WinSize | INTEGER | RW
.7 | PktSize | ENUM | RW
.8 | ShortHold | INTEGER | RW
.9 | MaxRetries | INTEGER | RW
.10 | BlockTime | INTEGER | RW
.11 | Addr | DisplayString | RW
.12 | Mode | ENUM | RW
.13 | AutoRoute | ENUM | RW
.14 | IpSubnet | IpAddress | RW
.15 | IpSubnetMask | IpAddress | RW
IfIndex
This object contains an interface index and assigns the row to an entry in ifTable. When creating new entries in the table, the value of this object shall be set to 0. The next free ifIndex value is than allocated by the BRICK and assigned to the object. At the same time a new interface is created in the IfTable.
Mtu
The Maximum transfer unit to be used with the interface, the row is describing. Range: 576 to 8180
Encapsulation
This object specifies the encapsulation method to be used. If this object is set to ip_rfc877, the RFC877 compatible encapsulation is selected. The relating interface is only capabable of transferring IP datagrams. All other protocols are not supported. Virtual channels are established only with the CUD field set to CC. If this object is set to ip, the relating interface is also only capable of forwarding IP datagrams. However, the virtual channels are setup with the CUD field set to 80 00 00 00 08 00. The encapsulation ipx allows only forwarding of IPX datagrams. VCs are established using a CUD field of 80 00 00 00 81 37. If this object is set to mpr, the corresponding corresponding interface is capable of IP, IPX and BRIDGING. The different protocols are multiplexed over the same VC. The CUD field is set to 00. Enumerations: ip-rfc877 (1) ip (2) ipx (3) mpr (4) delete (5)
NumVC
This object specifies the number of VCs used with the corresponding interface. The BRICK will always try to have that many VCs available for the relating interface. Range: 0 to 255
MaxVC
This object specifies the maximum number of VCs used with the corresponding interface. It shall be greater or equal to x25MprNumVC. Range: 0 to 255
WinSize
This object describes the window size to be used for outgoing X.25 virtual calls. Range: 1 to 7
PktSize
This object describes the packet size, to be used for outgoing X.25 calls. Please note that this parameter is independant of the x25MprMtu parameter. Enumerations: p128 (7) p256 (8) p512 (9) p1024 (10) p2048 (11) p4096 (12)
ShortHold
This object specifies the time of inactivity in seconds, after which the VCs are disconnected automatically. Range: 0 to 65535
MaxRetries
This object specifies the maximum number of tries for X.25 call establishement. If the BRICK has tried to establish the call for this many times, the interface is in the blocked state for a time specified by x25MprBlockTime. During the blocked state, no more tries are made. Range: 1 to 255
BlockTime
This object describes the amount of time, the corresponding interface remains in the blocked state after too many tries to establish the X.25 call. Range: 0 to 65536
Addr
The X.25 address to be used with this interface. A leading @ indicates extended adressing. Length: 0 to 255
Mode
This object describes the operating mode of the interface. normal -- normal operating mode multiuser -- A new interface is created for each incoming X.25 call. Enumerations: normal (1) multiuser (2)
AutoRoute
This object describes, how automatic routes are created. It is especially usefull combined with the multiuser Mode of the interface. off -- do not create automatic routes check -- Check the source address of the the first packet and create a backward Route, when in the range specified by IpSubnet/IpSubnetMask translate -- Translate the ip source address to the range specified by IpSubnet/IpSubnetMask. Automatically create ipNatOutEntries and set ipExtIfNat for dynamic interfaces to reverse. Enumerations: off (1) check (2) translate (3)
IpSubnet
This object specifies, together with x25MprSubnetMask the possible range for automatically created routes. The object is valid, when x25MprMode is set to autoroute or multiuser.
IpSubnetMask
This object specifies, together with x25MprSubnet the possible range for automatically created routes. The object is valid, when x25MprMode is set to autoroute or multiuser.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH