>> MIB - Management Information Base
>> Table: mpsExtensionSourceTable - (.1.3.6.1.4.1.272.4.53.6.4.1)
Description: This table contains the outgoing CLIP information for each subscriber, that will be displayed to the public exchange for external outgoing calls.
mpsExtensionSourceTable
OID | Name | Type | Access
.1 | Extension | ExtensionIndex | RW
.2 | TrunkGroup | TrunkGroupIndex | RW
.3 | SubscriberNumber | SubscriberNumberIndex | RW
.4 | SubscriberAdminStatus | ENUM | D
.5 | TrunkNumber | TrunkNumberIndexOrZero | RW
.6 | HideNumber | ENUM | RW
.7 | Type | ENUM | RW
.8 | Prio | Unsigned32 | RW
Extension
This variable references the mpsExtensionIndex. Range: 1 to 65535
TrunkGroup
This variable references the mpsTrunkGroupIndex. Range: 1 to 65535
SubscriberNumber
A unique value for each extension and outgoing external number.
SubscriberAdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
TrunkNumber
A unique value for each extension and outgoing external number. Index in mpsTrunkNumberTable Range: 0 to 65535
HideNumber
Always hide this number on outgoing calls from this subscriber. Enumerations: true (1) false (2)
Type
This variable contains the actual number signaling type. standard: standard number signaling -> use the number which is indexed via the mpsExtensionSourceTrunkNumber field. If this field is zero then no number signaling applies. In this case the public exchange/ provider may insert the default assigned number. own-ddi: extension number signaling -> use extension- + base number for DDI signaling Enumerations: standard (1) own-ddi (2)
Prio
Priority of the outgoing trunk number. Used to set the outgoing trunk line sequence individually for each extension (instead of globally via the ClassOfService).

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH