>> MIB - Management Information Base
>> Table: mpsNetworkTable - (.1.3.6.1.4.1.272.4.53.8.1.1)
Description: This table contains information for each IP location. Every VoIP extension and VoIP provider will be associate to an IP location.
mpsNetworkTable
OID | Name | Type | Access
.1 | Index | NetworkIndex | RW
.2 | RegTimer | INTEGER | RW
.3 | BwUpstream | INTEGER | RW
.4 | BwDownstream | INTEGER | RW
.5 | Address | IpAddress | RW
.6 | NetMask | IpAddress | RW
.7 | Descr | DisplayString | RW
.8 | Domain | DisplayString | RW
.9 | RTPTrafficReservation | INTEGER | RW
.10 | AdminStatus | ENUM | D
.11 | IfIndex | InterfaceIndexOrZero | RW
Index
A unique value for each location. Range: 1 to 18
RegTimer
Registration timer in seconds for IP extension. Set to 0 to get the time from the terminal.
BwUpstream
Bandwidth for upstream data in kBits/s.
BwDownstream
Bandwidth for downstream data in kBits/s.
Address
IP Address of the location.
NetMask
Subnet mask.
Descr
Name of the location. Length: 0 to 32
Domain
DNS name of the location. Length: 0 to 255
RTPTrafficReservation
Maximum RTP Traffic in percent.
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
IfIndex
Index of network interface from ifTable to apply the bandwidth settings. If the default value has been set, the entry is manually configured by the user otherwise automatic by the system. Range: 0 to 2147483647

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH