>> MIB - Management Information Base
>> Table: tr069LANDeviceXrefTable - (.1.3.6.1.4.1.272.4.22.6.2.10.1)
Description: An entry containing a cross reference between a LANDevice and associated local table entries.
tr069LANDeviceXrefTable
OID | Name | Type | Access
.1 | DeviceIdx | INTEGER | RW
.2 | EthConfigIdx | INTEGER | RW
.3 | EthIfIndex | INTEGER | RW
.4 | HostCfgIfIndex | INTEGER | RW
.5 | DHCPServerConfigurable | ENUM | RW
.6 | WLANConfigIdx | INTEGER | RW
.7 | WLANIfIndex | INTEGER | RW
.8 | XMLTreeState | ENUM | D
DeviceIdx
Index of this LAN device as presented to TR-069. Range: 0 to 2147483647
EthConfigIdx
Index of this EthernetInterfaceConfig as presented to TR-069. A value of 0 is used to indicate the absence of an Ethernet device.
EthIfIndex
Interface identifier representing one ethernet interface associated with this entry. A value of 0 is used to indicate the absence of an Ethernet device.
HostCfgIfIndex
Identifier representing the interface that carries the IP configuration associated with this entry.
DHCPServerConfigurable
Whether the LAN side DHCP server is configured by the ACS. Enumerations: false (1) true (2)
WLANConfigIdx
Index of this WLANConfiguration as presented to TR-069. A value of 0 is used to indicate the absence of a WLAN device.
WLANIfIndex
Identifier representing one WLAN interface associated with this entry. A value of 0 is used to indicate the absence of a WLAN device.
XMLTreeState
Whether this entry is present in the XML tree. Enumerations: setup (1) new (2) present (3) purge (4) delete (5)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH