>> MIB - Management Information Base
>> Table: qosIfStatTable - (.1.3.6.1.4.1.272.4.27.2.1)
Description: The qosIfStatTable contains statistical QoS-specific information for the interface specified by qosIfStatIndex (interface index). Only the system can add or delete entries to this table.
qosIfStatTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | OutPkts | Counter32 | R
.6 | PktsQueued | Counter32 | R
.7 | OctetsQueued | Counter32 | R
.8 | PktsDropped | Counter32 | R
.10 | State | ENUM | RW
.11 | TxRate | INTEGER | R
.12 | CurrVoipCalls | INTEGER | R
.13 | HCOutOctets | Counter64 | R
.14 | HCOctetsDropped | Counter64 | R
Index
The unique interface index.
OutPkts
The number of packets transmitted on the related interface since its last change to the 'up' state.
PktsQueued
The number of data packets enqueued and waiting to be sent across the related interface.
OctetsQueued
The amount of data (in octets) enqueued waiting to be sent across the related interface.
PktsDropped
The number of data packets dropped during congestion.
State
This object allows statistics to be reinitialized. Possible values: running(1) = no reset of statistics reset(2) = reset all counters in this entry except counters for queued packets and octets. resetall(3) = perform the same action as reset(2) and additionally perform reset action on associated entries of the qosPolicyStatTable and qosTosStatTable for the same interface. When the reset action is over, this object is automatically restored to its 'running(1)' default state. Enumerations: running (1) reset (2) resetall (3)
TxRate
The upload speed (amount of bits per second) of the associated interface.
CurrVoipCalls
The current number of VoIP Calls routed via the associated interface. Range: 0 to 64
HCOutOctets
The number of octets transmitted on the related interface since its last change to the 'up' state.
HCOctetsDropped
The representation of qosIfStatPktsDropped in octets.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH