>> MIB - Management Information Base
>> Table: adslAtucChanTable - (.1.3.6.1.4.1.272.4.30.1.1.4.1)
Description: An entry in the adslAtucChanTable.
adslAtucChanTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | InterleaveDelay | INTEGER | R
.3 | CurrTxRate | INTEGER | R
.4 | PrevTxRate | INTEGER | R
.5 | InterleaveDepth | INTEGER | R
IfIndex
Specifies the ADSL interface index.
InterleaveDelay
Interleave Delay for this channel. Interleave delay applies only to the interleave channel and defines the mapping (relative spacing) between subsequent input bytes at the interleaver input and their placement in the bit stream at the interleaver output. Larger numbers provide greater separation between consecutive input bytes in the output bit stream allowing for improved impulse noise immunity at the expense of payload latency. In the case where the ifType is Fast(125), use noSuchObject.
CurrTxRate
Actual transmit rate on this channel.
PrevTxRate
The rate at the time of the last adslAtucRateChangeTrap event. It is also set at initialization to prevent a trap being sent. Rate changes less than adslAtucThresh(*)RateDown or less than adslAtucThresh(*)RateUp will not cause a trap or cause this object to change. (*) == Fast or Interleave. See AdslLineAlarmConfProfileEntry.
InterleaveDepth
The interleaver depth.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH