>> MIB - Management Information Base
>> Table: apDiscTable - (.1.3.6.1.4.1.272.4.49.2.1)
Description: An entry for a discovered access point.
apDiscTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Proto | ENUM | R
.3 | MacAddress | MacAddress | R
.4 | NodeName | DisplayString | R
.5 | IpStatus | ENUM | R
.6 | IpAddress | IpAddress | R
.7 | NetMask | IpAddress | R
.8 | GwAddress | IpAddress | R
.9 | LastChange | Date | R
.10 | SerialNumber | DisplayString | R
.11 | SysDescription | DisplayString | R
.12 | VersionString | DisplayString | R
IfIndex
The interface on which the access point was detected. The interface is identified by its interface index in the ifTable.
Proto
This indicates via which discovery protocol the access point was found. Currently only the protocol to discover ARtem access points is supported. This is protocol uses IP multicast protocol with group address 239.239.239.239 and UPD port 1111. Enumerations: artem (1)
MacAddress
The MAC address of the found access point. The ARtem access points report via the discovery protocol the MAC address of their first ethernet-like interface. Length: 6 to 6
NodeName
The node name of the access point. Length: 0 to 32
IpStatus
This indicates how the access point got its IP address, netmask and gateway address. 'unknown' means that the access point does not give an indication how these values have been set, 'static' indicates that the values have been set statically or manually, 'dhcpLease' means that the values have been set via DHCP, 'dhcpFailed' means that DCHP request failed. Enumerations: unknown (1) static (2) dhcpLease (3) dhcpFailed (4)
IpAddress
The IP address of the access point.
NetMask
The netmask of the access point.
GwAddress
The gateway address of the access point.
LastChange
The time (GMT) when the access point was initially discovered or has changed its networking configuration given in seconds since 01/01/1970 00:00:00. Range: 0 to -1
SerialNumber
The serial number of the access point. Length: 0 to 32
SysDescription
The system description of the access point. Length: 0 to 64
VersionString
The version string of the access point. Length: 0 to 64

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH