>> MIB - Management Information Base
>> Table: dot11PhyTxPowerTable - (.1.2.840.10036.4.3.1)
Description: An entry in the dot11PhyTxPower Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11PhyTxPowerTable
OID | Name | Type | Access
.1 | NumberSupportedPowerLevels | INTEGER | R
.2 | TxPowerLevel1 | INTEGER | R
.3 | TxPowerLevel2 | INTEGER | R
.4 | TxPowerLevel3 | INTEGER | R
.5 | TxPowerLevel4 | INTEGER | R
.6 | TxPowerLevel5 | INTEGER | R
.7 | TxPowerLevel6 | INTEGER | R
.8 | TxPowerLevel7 | INTEGER | R
.9 | TxPowerLevel8 | INTEGER | R
.10 | CurrentTxPowerLevel | INTEGER | RW
NumberSupportedPowerLevels
The number of power levels supported by the PMD. This attribute can have a value of 1 to 8. Range: 1 to 8
TxPowerLevel1
The transmit output power for LEVEL1 in mW. This is also the default power level. Range: 0 to 10000
TxPowerLevel2
The transmit output power for LEVEL2 in mW. Range: 0 to 10000
TxPowerLevel3
The transmit output power for LEVEL3 in mW. Range: 0 to 10000
TxPowerLevel4
The transmit output power for LEVEL4 in mW. Range: 0 to 10000
TxPowerLevel5
The transmit output power for LEVEL5 in mW. Range: 0 to 10000
TxPowerLevel6
The transmit output power for LEVEL6 in mW. Range: 0 to 10000
TxPowerLevel7
The transmit output power for LEVEL7 in mW. Range: 0 to 10000
TxPowerLevel8
The transmit output power for LEVEL8 in mW. Range: 0 to 10000
CurrentTxPowerLevel
The TxPowerLevel N currently being used to transmit data. Some PHYs also use this value to determine the receiver sensitivity requirements for CCA. Range: 1 to 8

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH