>> MIB - Management Information Base
>> Table: mpsGroupModeChainTable - (.1.3.6.1.4.1.272.4.53.5.3.1)
Description: This table contains the extension in each group and Mode.
mpsGroupModeChainTable
OID | Name | Type | Access
.1 | Group | GroupIndex | RW
.2 | GroupMode | GroupModeIndex | RW
.3 | Position | Unsigned32 | RW
.4 | Extension | ExtensionIndexOrZero | RW
.5 | AdminStatus | ENUM | D
.6 | ExternalNumber | DisplayString | RW
Group
A unique value for each group, reference to mpsGroupTable and mpsGroupModeTable. Range: 1 to 99
GroupMode
A unique value for each Mode, reference to mpsGroupModeTable (same as mpsGroupModeNumber). Range: 1 to 10
Position
A unique value for each priority.
Extension
A unique value for each extension, reference to mpsExtensionTable. For further implementations this variable contains the reference to an mpsExtension entry or 0, to determine internal and external group members. Different membership: 1.) External member (mpsGroupModeChainExternalNumber = a valid external number) && (mpsGroupModeChainExtension = 0) 2.) Internal member (mpsGroupModeChainExternalNumber = empty string) && (mpsGroupModeChainExtension != 0) 3.) Internal member (mpsGroupModeChainExternalNumber = a valid external number) && (mpsGroupModeChainExtension != 0) 4.) Invalid entry (mpsGroupModeChainExternalNumber = empty string) && (mpsGroupModeChainExtension = 0) Range: 0 to 65535
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
ExternalNumber
For further implementations in this variable contains external numbers. To show that the mpsGroupModeChainEntry is assigned to an external team member, the mpsGroupModeChainExtension must be set to 0. Length: 0 to 20

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH