>> MIB - Management Information Base
>> Table: ipBodRuleTable - (.1.3.6.1.4.1.272.4.5.21.1)
Description: The ipBodRuleTable defines access rules for checking incoming IP packets. The rules are processed in order, i.e. each rule has a link to the next rule. The set of rules is processed until a match occurs, that means the rule's associated filter matches and the specified action is performed (either request or deny additional bandwidth). The last rule is implicitly a deny rule. The set of rules to be processed can be defined for each interface.
ipBodRuleTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | FilterIndex | INTEGER | R
.3 | Action | ENUM | D
.4 | Direction | ENUM | RW
.5 | Channels | INTEGER | RW
.6 | NextRuleIndex | INTEGER | RW
.7 | IdleTime | INTEGER | RW
Index
Unique rule index.
FilterIndex
References the rule's associated filter.
Action
This object specifies the action to be performed if the rule's associated filter matches. If set to ignore the filter is not consulted and the next rule is processed immediately. Enumerations: invoke (1) invoke-if-not (2) deny (3) deny-if-not (4) ignore (5) delete (6)
Direction
This object specifies the direction of the packets for which the rule is processed. Enumerations: outgoing (1) incoming (2) both (3)
Channels
The number of B-channels to invoke if the rule's associated filter matches. Range: 0 to 8
NextRuleIndex
Specifies the next rule to be processed if the rule's associated filter does not match. The value 0 is used to mark the end of the rule set.
IdleTime
Specifies the time in seconds the interface-specific shorthold interval (see biboPPPTable) is extended if the rule's associated filter matches. When set to zero this setting is ignored. When set to -1 matching packets are sent piggyback, they are not considered for shorthold mode. Range: -1 to 3600

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH