>> MIB - Management Information Base
>> Table: ipPublishTable - (.1.3.6.1.4.1.272.4.5.24.1)
Description: This entry contains all data for managing one dynamic DNS account hosted by a provider which is defined in one entry of the ipDynDnsProviderTable.
ipPublishTable
OID | Name | Type | Access
.1 | Perm | ENUM | D
.2 | Service | ENUM | RW
.3 | Status | ENUM | RW
.4 | Interface | INTEGER | RW
.5 | User | DisplayString | RW
.6 | Password | DisplayString | RW
.7 | IPAddress | IpAddress | R
.8 | LastUpdate | Date | R
.9 | Retries | INTEGER | RW
.20 | DynProvider | INTEGER | RW
.21 | DynHostName | DisplayString | RW
.23 | DynWild | ENUM | RW
.24 | DynMX | DisplayString | RW
.25 | DynCheckDNS | DisplayString | RW
.26 | Description | DisplayString | RW
Perm
Controls the use of this dynamic DNS entry. Enumerations: enabled (1) disabled (2) delete (3)
Service
Uses LDAP or dynamic DNS protocol for IP Publishing. Enumerations: ldap (1) dyndns (2)
Status
The actual status of the publishing procedure. Enumerations: failed (1) update (2) updating (3) checking (4) up-to-date (5)
Interface
The interface corresponding to this entry.
User
The user identification for dynamic DNS ip address updates. Length: 0 to 255
Password
The password for the dynamic DNS service authentication. Length: 0 to 255
IPAddress
The ip address which has been published last time.
LastUpdate
The timestamp of the last ip address update. Range: 0 to -1
Retries
The # of retries if the update of the actual ip address fails.
DynProvider
The index of the dynamic DNS provider in the ipDynDnsProviderTable. Range: 0 to 10000
DynHostName
The hostname of the dynamic DNS service provider for ip address updates. Length: 0 to 255
DynWild
Enable or disable the use of Wildcards (provider specific). Enumerations: off (1) on (2)
DynMX
The mx info (provider specific). Length: 0 to 255
DynCheckDNS
The official DNS server of the provider to use for verification of the updated ip address (currently unused). Length: 0 to 255
Description
A textual string describing this dynDNS client entry. Length: 0 to 255

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH