>> MIB - Management Information Base
>> Table: mpsArsRoutingConfig - (.1.3.6.1.4.1.272.4.53.10.1)
mpsArsRoutingConfig
OID | Name | Type | Access
.1 | Level | INTEGER | RW
.2 | Action | ENUM | RW
Level
This variable contains the maximum fallback level. Range: 0 to 2
Action
This value determine if fallback is enabled (true) or disabled (false). Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH