>> MIB - Management Information Base
>> Table: ipHostAccessClientTable - (.1.3.6.1.4.1.272.4.5.62.2.1)
Description: An entry representing a client on a particular interface which has requested host access authentication.
ipHostAccessClientTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | User | DisplayString | R
.3 | Password | DisplayString | N
.4 | Addr | IpAddress | R
.5 | PhysAddr | PhysAddress | R
.6 | Logon | Date | R
.7 | Expires | Date | R
.8 | AdminStatus | ENUM | D
.9 | MaxTransfer | Counter64 | R
.10 | InPkts | Counter64 | R
.11 | OutPkts | Counter64 | R
.12 | InOctets | Counter64 | R
.13 | OutOctets | Counter64 | R
.14 | LastAccountedRx | Date | R
.15 | LastAccountedTx | Date | R
.16 | LastWGardenRx | Date | R
.17 | LastWGardenTx | Date | R
.18 | LastLocalRx | Date | R
.19 | LastLocalTx | Date | R
.20 | LastAuthenticate | Date | R
.21 | LastAccounting | Date | R
.22 | ReportedInOctets | Counter64 | R
.23 | ReportedOutOctets | Counter64 | R
.24 | ReportedSessionTime | Unsigned32 | R
.25 | IdleTimeout | Unsigned32 | R
.26 | AcctInterval | Unsigned32 | R
.27 | SessionTimeReporting | ENUM | R
.28 | TerminateCause | Unsigned32 | R
.29 | NoReplyCounter | Unsigned32 | R
IfIndex
The interface index where the client is coming from.
User
The client's user name in upper/lower-case-writing as entered by the user. Please note that only one entry per user is allowed. The internal check for double-entries is done case-insensitively because many people use upper/lower-cases inconsistently. This must be considered also by the Radius-server-operator. Length: 0 to 255
Password
The client password. Length: 0 to 255
Addr
The client's IP address.
PhysAddr
The client's hardware address.
Logon
The time when the client has successfully authenticated. Valid only if ipHostAccessClientAdminStatus is NOT pending. Range: 0 to -1
Expires
The time when the client expires. 0 means NO expiry. Valid only if ipHostAccessClientAdminStatus is NOT pending. Range: 0 to -1
AdminStatus
The client-status is initialised to <pending>. After successful (initial) authentication, it is updated to <active>. Setting it to <delete> kills the related client-entry and triggers the final Radius-account-request. In case that a specific terminate-cause shall be reported, ipHostAccessClientTerminateCause must be set accordingly before triggering the <delete>. Enumerations: active (1) delete (2) pending (3)
MaxTransfer
Max. number of bytes this client can transfer. 0 means NO limit. Valid only if ipHostAccessClientAdminStatus is NOT pending.
InPkts
Current number of incoming packets for this client. Valid only if ipHostAccessClientAdminStatus is NOT pending.
OutPkts
Current number of outgoing packets for this client. Valid only if ipHostAccessClientAdminStatus is NOT pending.
InOctets
Current number of incoming octets for this client. Valid only if ipHostAccessClientAdminStatus is NOT pending.
OutOctets
Current number of outgoing octets for this client. Valid only if ipHostAccessClientAdminStatus is NOT pending.
LastAccountedRx
Timestamp of latest in-packet: accounted-remote->client Valid only if ipHostAccessClientAdminStatus is NOT pending. Range: 0 to -1
LastAccountedTx
Timestamp of latest out-packet: client->accounted-remote Valid only if ipHostAccessClientAdminStatus is NOT pending. Range: 0 to -1
LastWGardenRx
Timestamp of latest in-packet: walled-garden->client Valid only if ipHostAccessClientAdminStatus is NOT pending. Range: 0 to -1
LastWGardenTx
Timestamp of latest out-packet: client->walled-garden Valid only if ipHostAccessClientAdminStatus is NOT pending. Range: 0 to -1
LastLocalRx
Timestamp of latest in-packet: router->client Valid only if ipHostAccessClientAdminStatus is NOT pending. Range: 0 to -1
LastLocalTx
Timestamp of latest out-packet: client->router Valid only if ipHostAccessClientAdminStatus is NOT pending. Range: 0 to -1
LastAuthenticate
Timestamp of latest access-request. Range: 0 to -1
LastAccounting
Timestamp of latest accounting-request. Valid only if ipHostAccessClientAdminStatus is NOT pending. Range: 0 to -1
ReportedInOctets
Latest reported number of incoming octets for this client. Valid only if ipHostAccessClientAdminStatus is NOT pending.
ReportedOutOctets
Latest reported number of outgoing octets for this client. Valid only if ipHostAccessClientAdminStatus is NOT pending.
ReportedSessionTime
Latest reported session-time in seconds. Valid only if ipHostAccessClientAdminStatus is NOT pending.
IdleTimeout
The idle-timeout-period in seconds that is used for the client (coming from Radius-server or from default-value). In deviation from RFC 2865, section 5.28, a value of 0 is interpreted as NO idle-timeout. Valid only if ipHostAccessClientAdminStatus is NOT pending.
AcctInterval
The accounting-interim-interval in seconds that is used for the client (coming from Radius-server or from default-value). In deviation from RFC 2869, section 5.16, a value of 0 is interpreted as NO interim-updates. Valid only if ipHostAccessClientAdminStatus is NOT pending.
SessionTimeReporting
Copied from related ipHostAccessSessionTimeReporting entry. This avoids complications when this field is toggled. Enumerations: with-idle-time (1) without-idle-time (2)
TerminateCause
The accounting-terminate-cause as described in RFC 2866, section 5.10. See ipHostAccessClientAdminStatus for more details. If not set explicitly, <Lost Service> is used as default-value.
NoReplyCounter
This counter is initialised to 0 and increased whenever re-authentication fails because of no reply (e.g. because WAN down or server too slow). It is reset whenever re-authentication succeeds. When the counter reaches the limit that is specified by ipHostAccessReAuthenticateTries, the client is removed.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH