>> MIB - Management Information Base
>> Table: sysStat - (.1.3.6.1.4.1.272.4.17.500)
sysStat
OID | Name | Type | Access
.1 | BootConfig | ENUM | R
.2 | FunctionState | ENUM | R
BootConfig
After system boot this variable shows which configuration was loaded: none: no configuration whatsoever bootfac: factory boot configuration default: default configuration as provided by image boot: configuration found in flash. Enumerations: none (1) bootfac (2) default (3) boot (4)
FunctionState
This variable contains the current function state, which is toggeled by pressing the function button on the device. Enumerations: on (1) off (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH