>> MIB - Management Information Base
>> Table: dot11PhyERPTable - (.1.2.840.10036.4.14.1)
Description: An entry in the dot11PhyERPEntry Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11PhyERPTable
OID | Name | Type | Access
.1 | ERPPBCCOptionImplemented | ENUM | R
.2 | ERPBCCOptionEnabled | ENUM | RW
.3 | DSSSOFDMOptionImplemented | ENUM | R
.4 | DSSSOFDMOptionEnabled | ENUM | RW
.5 | ShortSlotTimeOptionImplemented | ENUM | RW
.6 | ShortSlotTimeOptionEnabled | ENUM | RW
ERPPBCCOptionImplemented
This attribute, when true, shall indicate that the ERPPBCC modulation option as defined in 19.6 is implemented. The default value of this attribute is false. Enumerations: true (1) false (2)
ERPBCCOptionEnabled
This attribute, when true, shall indicate that the ERPPBCCoption as defined in 19.6 is enabled. The default value of this attribute is false. Enumerations: true (1) false (2)
DSSSOFDMOptionImplemented
This attribute, when true, shall indicate that the DSSS-OFDM option as defined in 19.7 is implemented. The default value of this attribute is false. Enumerations: true (1) false (2)
DSSSOFDMOptionEnabled
This attribute, when true, shall indicate that the DSSS-OFDM option as defined in 19.7 is enabled. The default value of this attribute is false. Enumerations: true (1) false (2)
ShortSlotTimeOptionImplemented
This attribute, when true, shall indicate that the Short Slot Time option as defined in 7.3.1.4 is implemented. The default value of this attribute is false. Enumerations: true (1) false (2)
ShortSlotTimeOptionEnabled
This attribute, when true, shall indicate that the Short Slot Time option as defined in 7.3.1.4 is enabled. The default value of this attribute is false. Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH