>> MIB - Management Information Base
>> Table: mpsTrunkNumberModeTable - (.1.3.6.1.4.1.272.4.53.3.9.1)
Description: This table contains reroute information for each trunk number and mode.
mpsTrunkNumberModeTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | RW
.2 | NumberIndex | TrunkNumberIndex | RW
.3 | Mode | Unsigned32 | RW
.4 | RerouteIndex | ReRouteIndexOrZero | RW
.5 | AdminStatus | ENUM | D
Index
A unique value for each entry.
NumberIndex
This variable contains the trunk number index. Reference to mpsTrunkNumberTable. Range: 1 to 65535
Mode
For each trunk number index (mpsTrunkNumberModeNumberIndex), several modes can exists.
RerouteIndex
Index of the ReRouting function in mpsReRouteTable. 0 = ReRouting function deactived. Range: 0 to 65535
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH