>> MIB - Management Information Base
>> Table: capiListenTable - (.1.3.6.1.4.1.272.4.7.2.1)
Description: The capiListenTable contains the listen settings for each CAPI application. Creating entries: Entries can only be created by the system and is performed automatically upon receiving a CAPI_LISTEN_REQ message. Deleting entries: Entries are automatically removed by the system once the application releases.
capiListenTable
OID | Name | Type | Access
.1 | Application | INTEGER | R
.2 | Controller | HexValue | R
.3 | ServiceMask | HexValue | R
.4 | EazMask | HexValue | R
.5 | InfoMask | HexValue | R
.6 | CipMask | HexValue | R
.7 | CipMask2 | HexValue | R
Application
The application-number (capiApplNumber).
Controller
The ISDN controller number. This value refers to the isdnStkNumber. Range: 0 to -1
ServiceMask
The bit mask of CAPI 1.1 listen services. Specifies which 1TR6 services to listen for (CAPI 1.1 only). Range: 0 to -1
EazMask
The bit mask of CAPI 1.1 listen-EAZs (CAPI 1.1 only). Range: 0 to -1
InfoMask
The bit mask of the CAPI 1.1/2.0 listen InfoMask setting. The purpose of infomask is to specify the type of information for a physical connection or controller which will be provided by CAPI. Range: 0 to -1
CipMask
The bit mask of CAPI 2.0 listen CIPMask. The purpose of the CIPMask parameter is to select basic classes of incoming calls. CAPI 2.0 applications only. Range: 0 to -1
CipMask2
The bit mask of CAPI 2.0 listen CIPMask. Range: 0 to -1

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH