>> MIB - Management Information Base
>> Table: pppoeAcServiceTable - (.1.3.6.1.4.1.272.4.24.4.1)
Description: The pppoeAcServiceTable is used to specify the supported PPPoE service on the associated Ethernet interface. It's only relevant for the PPPoE server mode. Creating entries: Entries are added by the user. Deleting entries: Entries are removed once the respective variable pppoeAcServiceStatus is set to delete(3).
pppoeAcServiceTable
OID | Name | Type | Access
.1 | EthIfIndex | INTEGER | RW
.2 | Name | DisplayString | RW
.3 | Status | ENUM | D
EthIfIndex
The interface index (ifIndex) of the associated Ethernet interface.
Name
The accepted PPPoE SERVICE-NAME for PPPoE Active Discovery Offer (PADO) and PPPoE Active Discovery Session-confirmation (PADS) packets. Length: 0 to 255
Status
The administrative and operational status of this entry. If set to enabled(1), this entry will be considered for the PPPoE SERVICE-NAME check as described for the variable pppoeAcChkService. If set to disabled(2), this entry will be ignored. If set to delete(3), this entry will be removed. Enumerations: enabled (1) disabled (2) delete (3)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH