>> MIB - Management Information Base
>> Table: acctStoreTable - (.1.3.6.1.4.1.272.4.22.4.2.1)
Description: (one entry of acctStoreTable)
acctStoreTable
OID | Name | Type | Access
.1 | Type | ENUM | D
.2 | Content | ENUM | RW
.3 | Direction | ENUM | RW
.4 | Id | INTEGER | RW
.5 | Time | Date | RW
.6 | Info | DisplayString | RW
Type
Storage type of this entry. volatile : the entry is not saved permanent in flash permanent: the entry is saved permanent in flash delete : command to delete entries. Enumerations: volatile (1) permanent (2) delete (3)
Content
Content type of this entry. call : dialup call ifc : interface traffic summary the RX/TX-octets of the enabled interfaces are saved automatically each 10 min. The storage of appropriate interfaces is enabled with IP-Accouting in ipExtIfTable:Accounting Enumerations: call (1) ifc (2)
Direction
Direction type of this entry. in/out : for content call sum : summary entry (total call charge, ifc summary) Enumerations: in (1) out (2) sum (3)
Id
Entry-Id of the origin: content call: internal phone-number or UserId content ifc : interface index Range: 0 to 16777215
Time
Date and time of this entry creation Range: 0 to -1
Info
Accounting string. The fields are separated by ';' The fields are converted to following types: - Integer: 1-8 bytes length - String : must have leading ' ' (max length 15 chars) - BCD num: must have leading '.' (max length 30 digits) (e.g. phone number) e.g. 123;;456; Infostr;.091196730; Length: 0 to 255

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH