>> MIB - Management Information Base
>> Table: pimNbrSecAddressTable - (.1.3.6.1.4.1.272.4.5.54.2.1.3.1)
Description: An entry (conceptual row) in the pimNbrSecAddressTable.
pimNbrSecAddressTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | R
.2 | Type | ENUM | R
.3 | Primary | InetAddressIPv6 | R
.4 |  | InetAddressIPv6 | R
IfIndex
The value of ifIndex for the interface used to reach this PIM neighbor. Range: 1 to 2147483647
Type
The address type of this PIM neighbor. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Primary
The primary IP address of this PIM neighbor. The InetAddressType is given by the pimNbrSecAddressType object. Length: 16 to 16
The secondary IP address of this PIM neighbor. The InetAddressType is given by the pimNbrSecAddressType object. Length: 16 to 16

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH