>> MIB - Management Information Base
>> Table: mpsTrunkGroupPOTSTable - (.1.3.6.1.4.1.272.4.53.3.6.1)
Description: This table contains advanced information of the external pots trunk groups.
mpsTrunkGroupPOTSTable
OID | Name | Type | Access
.1 | Index | TrunkGroupIndex | RW
.2 | DialingType | ENUM | RW
.3 | Wait2Dial | INTEGER | RW
.4 | BusytoneDetection | ENUM | RW
.5 | BusytoneTimeSlice | INTEGER | RW
.6 | Clip | ENUM | RW
.7 | ChargeFrequency | ENUM | RW
.8 | EndOfDial | INTEGER | RW
.9 | AdminStatus | ENUM | D
.10 | FaxSwitchIndex | FaxSwitchIndexOrZero | RW
.11 | Uefs | ENUM | RW
Index
A unique value for each trunk group. Range: 1 to 65535
DialingType
Type of dialling, DTMF and pulse dialing. Enumerations: none (1) mfv (2) iwv (3)
Wait2Dial
Time slice in seconds, before digits will be send to trunk. Set to 0: dial tone detection is on.
BusytoneDetection
This value determine if busystone detection is on (true) or off (false). Enumerations: true (1) false (2)
BusytoneTimeSlice
Max time slice in seconds, to detect the busytone.
Clip
Number display (CLIP). Enumerations: none (1) mfv (2) dtmf (3)
ChargeFrequency
This value determine the frequency of the charge pulse for POTS trunk groups Enumerations: no (1) f12khz (2) f16khz (3)
EndOfDial
End of dial time slice in seconds.
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
FaxSwitchIndex
A unique value for each fax switch. Range: 0 to 65535
Uefs
This value determine if 'DDI on POTS' (UEFS) is on (true) or off (false). Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH