>> MIB - Management Information Base
>> Table: systemPhoneFacilityTable - (.1.3.6.1.4.1.272.4.64.1.3.1)
Description: This table contains system phone configuration concerning display and operations. An entry in this table will also be deleted if the related systemPhoneTable entry is deleted.
systemPhoneFacilityTable
OID | Name | Type | Access
.1 | Index | SystelTerminalIndex | RW
.2 | DisplayGeneral | BITS | RW
.3 | DisplayDuringCall | ENUM | RW
.4 | LedConf | ENUM | RW
.5 | DispLang | ENUM | RW
.6 | CharacterSet | ENUM | RW
.7 | AutoCallAcceptTime | ENUM | RW
.8 | CallWaitInt | ENUM | RW
.9 | CallWaitExt | ENUM | RW
.10 | DoNotDisturb | ENUM | RW
.11 | AdminStatus | ENUM | D
.12 | NGDisplayLight | ENUM | RW
.13 | NGDoNotDisturbTone | INTEGER | RW
.14 | NGLedConf | BITS | RW
Index
Reference to the mpsTerminalTable. Range: 1 to 65535
DisplayGeneral
Facility settings for display and operation control: softkey-style: (0) use of lower case, (1) use of upper case for the softkeys. clir: (0) activate number suppression (outgoing CLIR active), (1) deactivate number suppression (outgoing CLIP active). colr: (0) activate number suppression (incoming COLR active), (1) deactivate number suppression (incoming COLP active). call-end-info: Enable (1) or disable (0) displaying call information after call is disconnected. do-not-disturb: (0) the do not disturb option is true for all MSNs, (1) the do not disturb option is true for the first MSN only. softkey-local-phonebook: (0) enable softkey for PBX phonebook access, (1) enable softkey for local phonebook access. dial-option: (0) DTMF, (1) Keypad. uus-inhibit-ctrl-int: Enable (1) or disable (0) the UUS inhibit intern. uus-inhibit-ctrl-ext: Enable (1) or disable (0) the UUS inhibit extern. auto-call-accept: Enable (1) or disable (0) the automatic call acceptance with the configured settings of systemPhoneFacAutoCall- AcceptTime. (This bit is only used with NG system phones. Enumerations: softkey-style (0) clir (1) colr (2) call-end-info (3) do-not-disturb (4) softkey-local-phonebook (5) dial-option (6) uus-inhibit-ctrl-int (7) uus-inhibit-ctrl-ext (8) auto-call-accept (9)
DisplayDuringCall
Information shown on display during an active call: number-and-costOrDuration(1): Shows call number and cost, if no costs are provided by the PSTN instead the call number and the duration will be shown. number-and-costOrNothing(2): Shows call number and cost, if no costs are provided by the PSTN instead only call number will be shown. number-and-duration(3): Shows call number and duration. number-and-time(4): Shows call number and actual time. numberOnly(5): Shows call number only. date-and-time-only(6): Shows actual date and time only. Enumerations: number-and-costOrDuration (1) number-and-costOrNothing (2) number-and-duration (3) number-and-time (4) numberOnly (5) date-and-time-only (6)
LedConf
Information of status LED function for elmeg CS/IP series system phones: indication-off: Status LED function is off. indication-all: Status LED blinks on all new events. indication-message: Status LED blinks only if a new message received. Enumerations: indication-off (1) indication-all (2) indication-message (3)
DispLang
The current display language. Enumerations: german (1) dutch (2) english (3) italian (5) danish (6) spanish (7) swedish (8) french (10) portuguese (11) czech (14) norwegian (16) greek (17) icelandic (20) polish (21) hungarian (22) russian (23) romanian (24) slovak (25)
CharacterSet
The character set of the display language: latin-ext: Latin character set with extensions. latin-greek: Latin and greek character set. latin-cyrillic: Latin and cyrillic character set. Enumerations: latin-ext (1) latin-greek (2) latin-cyrillic (3)
AutoCallAcceptTime
Setting of automatic call acceptance time, only used if 'headset' in systemPhoneAudioFac is enabled(1) and a function-key 'autoanswer' is configured and active on the system phone. For NG phones there are new values available, marked with *: immediately: phone immediately accepts calls. sec-5: phone accepts calls after 5 seconds ringing. sec-10: phone accepts calls after 10 seconds ringing. sec-15: *phone accepts calls after 15 seconds ringing (only for NG phones). sec-20: *phone accepts calls after 20 seconds ringing (only for NG phones). Enumerations: immediately (1) sec-5 (2) sec-10 (3) sec-15 (4) sec-20 (5)
CallWaitInt
Setting for intern call waiting: off: call waiting signal is disabled. on: call waiting signal is activated (user is noticed by a single tone). Enumerations: off (1) on (2)
CallWaitExt
Setting for extern call waiting: off: call waiting signal is disabled. on: call waiting signal is activated (user is noticed by a single tone). Enumerations: off (1) on (2)
DoNotDisturb
Information of do not disturb setup: disable: Do not disturb option is disabled. quiet: Do not disturb option is enabled, without notice tone. notice: Do not disturb option is enabled, a single notice tone indicates an incoming call. Enumerations: disable (1) quiet (2) notice (3)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
NGDisplayLight
Settings for display light - this mib item is only important for NG system phones: sec-x: After an user action (e.g. keypress) display light is on for dedicated time x. always-off: Display light is always off. always-on: Display light is always on. Enumerations: sec-15 (1) sec-30 (2) sec-45 (3) sec-60 (4) sec-75 (5) sec-90 (6) sec-105 (7) sec-120 (8) sec-135 (9) always-off (64) always-on (128)
NGDoNotDisturbTone
Information of do not disturb setup for NG system phones: 0: NG system phone signals incoming calls/messages without any tone. 1..4: NG system phone signals incoming calls/messages with special tone. Note: If there is no configured do-not-disturb-key, there is no chance to activate the do not disturb option for NG system phones. Settings made in systemPhoneFacNGDoNotDisturb are only SETTINGS, activation or deactivation of do not disturb mode only is possibly via configured do not disturb key. Otherwise, if no key is configured, NG system phone always signals incoming calls with selected call melody. Range: 0 to 4
NGLedConf
Information of status LED function for NG system phones: new-message: Status LED blinks if new message received, new-call: Status LED blinks if call was missed, call-state: Status LED blinks in call state. Enumerations: message-received (0) call-received (1) call-state (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH