>> MIB - Management Information Base
>> Table: xotIfTable - (.1.3.6.1.4.1.272.4.32.1.1)
Description: Entries in this table are created by defining a new value for the field xotIfIndex. Entries may be deleted by setting the field xotIfAllowIncoming to the value delete.
xotIfTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | InIpAddr | IpAddress | RW
.3 | InIpMask | IpAddress | RW
.4 | OutIpAddr | IpAddress | RW
.5 | OutPort | INTEGER | RW
.6 | MaxLinks | INTEGER | RW
.7 | Mtu | INTEGER | RW
.8 | AllowIncoming | ENUM | D
.9 | SrcIpAddr | IpAddress | RW
Index
The index of the virtual interface. This object identifies a row in the ifTable.
InIpAddr
The IP address of remote partner by incoming calls.
InIpMask
The subnet mask associated with the IP address of remote partner by incoming calls. This indicates the mask to be logical-ANDed with the received source IP address before being compared to the value in the xotIfInIpAddr field.
OutIpAddr
The IP address of remote partner by outgoing calls.
OutPort
The port number of remote partner by outgoing calls. Range: 1 to 65535
MaxLinks
The Maximum number of Links. Range: 0 to 9999
Mtu
The Maximum transfer unit to be used with the interface. Range: 576 to 8180
AllowIncoming
This object indicates, whether incoming connection should be allowed on the link. Enumerations: yes (1) no (2) delete (3)
SrcIpAddr
The source IP address for outgoing calls.

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH