>> MIB - Management Information Base
>> Table: dot11RSNAConfigAuthenticationSuitesTable - (.1.2.840.10036.1.11.1)
Description: An entry (row) in the dot11RSNAConfigAuthenticationSuitesTable.
dot11RSNAConfigAuthenticationSuitesTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | R
.2 |  | OCTET STRING | R
.3 | Enabled | ENUM | RW
Index
The auxiliary variable used as an index into the dot11RSNAConfigAuthenticationSuitesTable. Range: 1 to -1
The selector of an AKM suite. It consists of an OUI (the first 3 octets) and a cipher suite identifier (the last octet). Length: 4 to 4
Enabled
This variable indicates whether the corresponding AKM suite is enabled/disabled. Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH