>> MIB - Management Information Base
>> Table: vlanTable - (.1.3.6.1.4.1.272.4.39.2.1)
Description: Each entry contains a unique virtIfIndex and the physical address used. The corresponding IP-Address musr be taken from the ipAddressTable.
vlanTable
OID | Name | Type | Access
.1 | Id | INTEGER | RW
.2 | Descr | OCTET STRING | RW
.3 | Status | ENUM | D
Id
VLAN Id. Range: 0 to 4095
Descr
Description of the VLAN. Length: 0 to 32
Status
Status of this entry. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH