>> MIB - Management Information Base
>> Table: dot11PhyHTTable - (.1.2.840.10036.4.15.1)
Description: An entry in the dot11PhyHTEntry Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11PhyHTTable
OID | Name | Type | Access
.1 | FortyMHzOperationImplemented | ENUM | R
.2 | FortyMHzOperationEnabled | ENUM | RW
.3 | CurrentPrimaryChannel | INTEGER | R
.4 | CurrentSecondaryChannel | INTEGER | RW
.5 | NumberOfSpatialStreamsImplemented | INTEGER | R
.6 | NumberOfSpatialStreamsEnabled | INTEGER | RW
.7 | GreenfieldOptionImplemented | ENUM | R
.8 | GreenfieldOptionEnabled | ENUM | RW
.9 | ShortGIOptionInTwentyImplemented | ENUM | R
.10 | ShortGIOptionInTwentyEnabled | ENUM | RW
.11 | ShortGIOptionInFortyImplemented | ENUM | R
.12 | ShortGIOptionInFortyEnabled | ENUM | RW
.13 | LDPCCodingOptionImplemented | ENUM | R
.14 | LDPCCodingOptionEnabled | ENUM | RW
.15 | TxSTBCOptionImplemented | ENUM | R
.16 | TxSTBCOptionEnabled | ENUM | RW
.17 | RxSTBCOptionImplemented | ENUM | R
.18 | RxSTBCOptionEnabled | ENUM | RW
.19 | BeamFormingOptionImplemented | ENUM | R
.20 | BeamFormingOptionEnabled | ENUM | RW
.21 | HighestSupportedDataRate | INTEGER | RW
.22 | TxMCSSetDefined | ENUM | RW
.23 | TxRxMCSSetNotEqual | ENUM | RW
.24 | TxMaximumNumberSpatialStreamsSupported | INTEGER | RW
.25 | TxUnequalModulationSupported | ENUM | RW
FortyMHzOperationImplemented
This attribute, when TRUE, indicates that the 40 MHz Operation is implemented. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
FortyMHzOperationEnabled
This attribute, when TRUE, indicates that the 40 MHz Operation is enabled. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
CurrentPrimaryChannel
This attribute indicates the operating channel. If 20/40 MHz Mode is currently in use then this attribute indicates the primary channel.
CurrentSecondaryChannel
This attribute indicates the channel number of the secondary channel. If 20/40 MHz mode is not currently in use, this attribute value shall be 0.
NumberOfSpatialStreamsImplemented
This attribute indicates the maximum number of spatial streams implemented. The default value of this attribute is 2. Range: 1 to 4
NumberOfSpatialStreamsEnabled
This attribute indicates the maximum number of spatial streams enabled. The default value of this attribute is 2. Range: 1 to 4
GreenfieldOptionImplemented
This attribute, when TRUE, indicates that the HT Greenfield option is implemented. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
GreenfieldOptionEnabled
This attribute, when TRUE, indicates that the HT Greenfield option is enabled. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ShortGIOptionInTwentyImplemented
This attribute, when TRUE, indicates that the Short Guard option is implemented for 20 MHz operation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ShortGIOptionInTwentyEnabled
This attribute, when TRUE, indicates that the Short Guard option is enabled for 20 MHz operation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ShortGIOptionInFortyImplemented
This attribute, when TRUE, indicates that the Short Guard option is implemented for 40 MHz operation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ShortGIOptionInFortyEnabled
This attribute, when TRUE, indicates that the Short Guard option is enabled for 40 MHz operation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
LDPCCodingOptionImplemented
This attribute, when TRUE, indicates that the LDPC coding option is implemented. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
LDPCCodingOptionEnabled
This attribute, when TRUE, indicates that the LDPC coding option is enabled. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TxSTBCOptionImplemented
This attribute, when TRUE, indicates that the entity is capable of transmitting frames using Space-Time Block Code (STBC) option. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TxSTBCOptionEnabled
This attribute, when TRUE, indicates that the entity's capability of transmitting frames using Space-Time Block Code (STBC) option is enabled. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
RxSTBCOptionImplemented
This attribute, when TRUE, indicates that the entity is capable of receiving frames that are sent using the Space-Time Block Code (STBC). The default value of this attribute is FALSE. Enumerations: true (1) false (2)
RxSTBCOptionEnabled
This attribute, when TRUE, indicates that the entity's capability of receiving frames that are sent using the Space-Time Block Code (STBC) is enabled. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
BeamFormingOptionImplemented
This attribute, when TRUE, indicates that the Beam Forming option is implemented. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
BeamFormingOptionEnabled
This attribute, when TRUE, indicates that the Beam Forming option is enabled. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
HighestSupportedDataRate
This attribute shall specify the Highest Data Rate in Mb/s at which the station may receive data. The default value of this attribute shall be 0. Range: 0 to 600
TxMCSSetDefined
This attribute, when TRUE, indicates that the Tx MCS set is defined. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TxRxMCSSetNotEqual
This attribute, when TRUE, indicates that the supported Tx and Rx MCS sets are not equal. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TxMaximumNumberSpatialStreamsSupported
This attribute indicates the Tx maximum number of spatial streams supported. The default value of this attribute is 0. Range: 0 to 3
TxUnequalModulationSupported
This attribute, when TRUE, indicates that Tx unequal modulation is supported. The default value of this attribute is FALSE. Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.10 generated on 2014/08/11. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH